| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3271: Machine instructions IMUL IMULB IMULW IMULD in 16bit mode

Tested procedures
  IigIMUL IigIMULB IigIMULW IigIMULD

Source & expected listing t3271.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=32, CPU=386 | |t3271 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:F6E9 | IMUL CL |0002:F7E9 | IMUL CX |0004:66F7E9 | IMUL ECX |0007:F62E[6600] | IMUL [MemByte] |000B:F72E[6400] | IMUL [MemWord] |000F:66F72E[6000] | IMUL [MemDword] |0014:F62C | IMUL [SI],DATA=BYTE |0016:F62C | IMULB [SI] |0018:F72C | IMUL [SI],DATA=WORD |001A:F72C | IMULW [SI] |001C:66F72C | IMUL [SI],DATA=DWORD |001F:66F72C | IMULD [SI] |0022:0FAFCA | IMUL CX,DX |0025:660FAFCA | IMUL ECX,EDX |0029:0FAF0C | IMUL CX,[SI] |002C:660FAF0C | IMUL ECX,[SI] |0030:69CA7EFF | IMUL CX,DX,-130 |0034:69CA7FFF | IMUL CX,DX,-129 |0038:6BCA80 | IMUL CX,DX,-128 |003B:6BCA81 | IMUL CX,DX,-127 |003E:6BCA7E | IMUL CX,DX,+126 |0041:6BCA7F | IMUL CX,DX,+127 |0044:69CA8000 | IMUL CX,DX,+128 |0048:69CA8100 | IMUL CX,DX,+129 |004C:6B0C03 | IMUL CX,[SI],3 |004F:690C0300 | IMUL CX,[SI],3,IMM=WORD |0053:666B0C03 | IMUL ECX,[SI],3 |0057:66690C03000000 | IMUL ECX,[SI],3,IMM=DWORD |005E:87C9 | ALIGN QWORD |0060:00000000 |MemDword DD D |0064:0000 |MemWord DW W |0066:00 |MemByte DB B | | ENDPROGRAM t3271`

Expected messages t3271.out
  `I0180 Assembling source file "t3271.htm". I0270 Assembling source "t3271". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3271". "t3271.htm"{58} I0510 Assembling program pass 1. "t3271.htm"{58} I0510 Assembling program pass 2. "t3271.htm"{58} I0510 Assembling program pass 3. "t3271.htm"{58} I0530 Assembling program pass 4 - final. "t3271.htm"{58} I0660 16bit TINY BIN file "t3271.bin" created, size=103. "t3271.htm"{92} I0650 Program "t3271" assembled in 4 passes with errorlevel 0. "t3271.htm"{92} I0750 Source "t3271" (112 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3271.htm.lst" created, size=1859. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲