| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t4550: Machine instructions VPCOMB VPCOMLTB VPCOMLEB VPCOMGTB VPCOMGEB VPCOMEQB VPCOMNEQB VPCOMFALSEB VPCOMTRUEB

Tested procedures
  IixVPCOMB IixVPCOMLTB IixVPCOMLEB IixVPCOMGTB IixVPCOMGEB IixVPCOMEQB IixVPCOMNEQB IixVPCOMFALSEB IixVPCOMTRUEB

Source & expected listing t4550.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=24,CPU=X64,SIMD=AVX,AMD=ON,XOP=ON,PROT=ON | |t4550 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:8FE868CCCB04 | VPCOMB XMM1,XMM2,XMM3,4 |00000006:8FE868CCCB00 | VPCOMLTB XMM1,XMM2,XMM3 |0000000C:8FE868CCCB01 | VPCOMLEB XMM1,XMM2,XMM3 |00000012:8FE868CCCB02 | VPCOMGTB XMM1,XMM2,XMM3 |00000018:8FE868CCCB03 | VPCOMGEB XMM1,XMM2,XMM3 |0000001E:8FE868CCCB04 | VPCOMEQB XMM1,XMM2,XMM3 |00000024:8FE868CCCB05 | VPCOMNEQB XMM1,XMM2,XMM3 |0000002A:8FE868CCCB06 | VPCOMFALSEB XMM1,XMM2,XMM3 |00000030:8FE868CCCB07 | VPCOMTRUEB XMM1,XMM2,XMM3 |00000036:8FE868CC0E04 | VPCOMB XMM1,XMM2,[RSI],4 |0000003C:8FE868CC0E00 | VPCOMLTB XMM1,XMM2,[RSI] |00000042:8FE868CC0E01 | VPCOMLEB XMM1,XMM2,[RSI] |00000048:8FE868CC0E02 | VPCOMGTB XMM1,XMM2,[RSI] |0000004E:8FE868CC0E03 | VPCOMGEB XMM1,XMM2,[RSI] |00000054:8FE868CC0E04 | VPCOMEQB XMM1,XMM2,[RSI] |0000005A:8FE868CC0E05 | VPCOMNEQB XMM1,XMM2,[RSI] |00000060:8FE868CC0E06 | VPCOMFALSEB XMM1,XMM2,[RSI] |00000066:8FE868CC0E07 | VPCOMTRUEB XMM1,XMM2,[RSI] | |ENDPROGRAM t4550`

Expected messages t4550.out
  `I0180 Assembling source file "t4550.htm". I0270 Assembling source "t4550". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t4550". "t4550.htm"{73} I0510 Assembling program pass 1. "t4550.htm"{73} I0530 Assembling program pass 2 - final. "t4550.htm"{73} I0660 16bit TINY BIN file "t4550.bin" created, size=108. "t4550.htm"{93} I0650 Program "t4550" assembled in 2 passes with errorlevel 0. "t4550.htm"{93} I0750 Source "t4550" (111 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t4550.htm.lst" created, size=1257. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲