| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t6122: Machine instructions VPSUBRD VPSBBRD VPMULHUD VPMULHD VFIXUPNANPS VPMADD231D VPADDSETSD

Tested procedures
  IiyVPSBBRD IiyVPSUBRD IiyVPMADD231D IiyVPMULHUD IiyVPMULHD IiyVFIXUPNANPS IiyVPADDSETSD

Source & expected listing t6122.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,MVEX=ON | |t6122 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F2690C6CCB | VPSUBRD ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=0 ; {dcba}. |00000006:62F2691C6CCB | VPSUBRD ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=1 ; {cdab}. |0000000C:62F2692C6CCB | VPSUBRD ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=2 ; {badc}. |00000012:62F2693C6CCB | VPSUBRD ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=3 ; {dacb}. |00000018:62F2694C6CCB | VPSUBRD ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=4 ; {aaaa}. |0000001E:62F2695C6CCB | VPSUBRD ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=5 ; {bbbb}. |00000024:62F2696C6CCB | VPSUBRD ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=6 ; {cccc}. |0000002A:62F2697C6CCB | VPSUBRD ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=7 ; {dddd}. |00000030:62F2690C6C4D01<6 | VPSUBRD ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=0 ; {16to16}. |00000037:62F2691C6C4D10<2 | VPSUBRD ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=1 ; {1to16}. |0000003E:62F2692C6C4D04<4 | VPSUBRD ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=2 ; {4to16}. |00000045:62F2694C6C4D04<4 | VPSUBRD ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=4 ; {uint8}. |0000004C:62F2695C6C4D04<4 | VPSUBRD ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=5 ; {sint8}. |00000053:62F2696C6C4D02<5 | VPSUBRD ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=6 ; {uint16}. |0000005A:62F2697C6C4D02<5 | VPSUBRD ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=7 ; {sint16}. |00000061:62F2690C6ECB | VPSBBRD ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=0 ; {dcba}. |00000067:62F2690C6E4D01<6 | VPSBBRD ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=0 ; {16to16}. |0000006E:62F2690C86CB | VPMULHUD ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=0 ; {dcba}. |00000074:62F2690C864D01<6 | VPMULHUD ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=0 ; {16to16}. |0000007B:62F2690C87CB | VPMULHD ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=0 ; {dcba}. |00000081:62F2690C874D01<6 | VPMULHD ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=0 ; {16to16}. |00000088:62F269CC55CB | VFIXUPNANPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=1,SAE=ON |0000008E:62F2690C554D01<6 | VFIXUPNANPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=0 ; {16to16}. |00000095:62F2693CB5CB | VPMADD231D ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=3 ; {dacb}. |0000009B:62F2690CB54D01<6 | VPMADD231D ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=0 ; {16to16}. |000000A2:62F2693CCDCB | VPADDSETSD ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=3 ; {dacb}. |000000A8:62F2690CCD4D01<6 | VPADDSETSD ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=0 ; {16to16}. |000000AF:62F2691CCD4D10<2 | VPADDSETSD ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=1 ; {1to16}. |000000B6:62F2692CCD4D04<4 | VPADDSETSD ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=2 ; {4to16}. | |ENDPROGRAM t6122`

Expected messages t6122.out
  `I0180 Assembling source file "t6122.htm". I0270 Assembling source "t6122". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t6122". "t6122.htm"{67} I0510 Assembling program pass 1. "t6122.htm"{67} I0530 Assembling program pass 2 - final. "t6122.htm"{67} I0660 16bit TINY BIN file "t6122.bin" created, size=189. "t6122.htm"{98} I0650 Program "t6122" assembled in 2 passes with errorlevel 0. "t6122.htm"{98} I0750 Source "t6122" (116 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t6122.htm.lst" created, size=2809. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲