| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5210: Machine instructions VADDSS,VADDSD,VMULSS,VMULSD,VSUBSS,VSUBSD,VDIVSS,VDIVSD

Tested procedures
  IizVADDSS IizVADDSD IizVMULSS IizVMULSD IizVSUBSS IizVSUBSD IizVDIVSS IizVDIVSD IizGroupVADDSS IizGroupVADDSD

Source & expected listing t5210.htm.lst
  `| |EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=30, CPU=X64, SIMD=AVX512, EVEX=ON | |t5210 PROGRAM WIDTH=64, FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[CODE] ::::Section changed. |00000000:C5EA580E | VADDSS XMM1,XMM2,[RSI] |00000004:62916E5C58CE | VADDSS XMM1,XMM2,XMM30,ROUND=UP,MASK=4 |0000000A:C5EB580E | VADDSD XMM1,XMM2,[RSI] |0000000E:6291EF5C58CE | VADDSD XMM1,XMM2,XMM30,ROUND=UP,MASK=4 |00000014:C5EA590E | VMULSS XMM1,XMM2,[RSI] |00000018:62916E5C59CE | VMULSS XMM1,XMM2,XMM30,ROUND=UP,MASK=4 |0000001E:C5EB590E | VMULSD XMM1,XMM2,[RSI] |00000022:6291EF5C59CE | VMULSD XMM1,XMM2,XMM30,ROUND=UP,MASK=4 |00000028:C5EA5C0E | VSUBSS XMM1,XMM2,[RSI] |0000002C:62916E5C5CCE | VSUBSS XMM1,XMM2,XMM30,ROUND=UP,MASK=4 |00000032:C5EB5C0E | VSUBSD XMM1,XMM2,[RSI] |00000036:6291EF5C5CCE | VSUBSD XMM1,XMM2,XMM30,ROUND=UP,MASK=4 |0000003C:C5EA5E0E | VDIVSS XMM1,XMM2,[RSI] |00000040:62916E5C5ECE | VDIVSS XMM1,XMM2,XMM30,ROUND=UP,MASK=4 |00000046:C5EB5E0E | VDIVSD XMM1,XMM2,[RSI] |0000004A:6291EF5C5ECE | VDIVSD XMM1,XMM2,XMM30,ROUND=UP,MASK=4 | |ENDPROGRAM t5210`

Expected messages t5210.out
  `I0180 Assembling source file "t5210.htm". I0270 Assembling source "t5210". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5210". "t5210.htm"{76} I0510 Assembling program pass 1. "t5210.htm"{76} I0530 Assembling program pass 2 - final. "t5210.htm"{76} I0660 64bit TINY BIN file "t5210.bin" created, size=80. "t5210.htm"{94} I0650 Program "t5210" assembled in 2 passes with errorlevel 0. "t5210.htm"{94} I0750 Source "t5210" (112 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5210.htm.lst" created, size=1304. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲