| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3203: Machine instructions XLAT XLATB

Tested procedures
  IigXLAT IigXLATB

Source & expected listing t3203.htm.lst
  `| | EUROASM DUMPWIDTH=24,CPU=X64 | |t3203 PROGRAM FORMAT=BIN,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:D7 | XLAT |0001:D7 | XLATB |0002:D7 | XLAT [BX] |0003:67D7 | XLAT [EBX] |0005:D7 | XLAT [DS:BX] |0006:3ED7 |SEGDS XLAT [BX] |0008:26D7 |SEGES:XLAT |000A:26D7 | XLAT [ES] |000C:26D7 | XLAT [ES:] |000E:26D7 | XLAT [ES:BX] |0010:2667D7 | XLAT [ES:EBX] |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:D7 | XLAT |00000001:D7 | XLATB |00000002:D7 | XLAT [EBX] |00000003:67D7 | XLAT [BX] |00000005:64D7 |SEGFS:XLAT |00000007:64D7 | XLAT [FS] |00000009:64D7 | XLAT [FS:] |0000000B:64D7 | XLAT [FS:EBX] |0000000D:6467D7 | XLAT [FS:BX] |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:D7 | XLAT |00000001:D7 | XLATB |00000002:D7 | XLAT [RBX] |00000003:67D7 | XLAT [EBX] |00000005:65D7 |SEGGS:XLAT [RBX] |00000007:65D7 | XLAT [GS:RBX] |00000009:6567D7 | XLAT [GS:EBX] | |ENDPROGRAM t3203`

Expected messages t3203.out
  `I0180 Assembling source file "t3203.htm". I0270 Assembling source "t3203". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3203". "t3203.htm"{52} I0510 Assembling program pass 1. "t3203.htm"{52} I0530 Assembling program pass 2 - final. "t3203.htm"{52} I0660 16bit TINY BIN file "t3203.bin" created, size=60. "t3203.htm"{83} I0650 Program "t3203" assembled in 2 passes with errorlevel 0. "t3203.htm"{83} I0750 Source "t3203" (101 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3203.htm.lst" created, size=1354. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲