| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3645: Machine instructions EMMS, FEMMS, MASKMOVQ, MOVNTQ , PINSRW, PMOVMSKB, PSHUFW

Tested procedures
  IimEMMS IidFEMMS IimMASKMOVQ IimMOVNTQ IimPINSRW IimPMOVMSKB IimPSHUFW

Source & expected listing t3645.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,FPU=ON,MMX=ON,D3NOW=ON,SIMD=SSE2,AMD=ON | |t3645 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF, IMAGEBASE=0 |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:0F77 | EMMS |0002:0F0E | FEMMS |0004:0FF7CF | MASKMOVQ MM1,MM7 |0007:0FF7CF | MASKMOVQ [DS:DI],MM1,MM7 |000A:260FF7CF | MASKMOVQ [ES:DI],MM1,MM7 |000E:670FF7CF | MASKMOVQ [EDI],MM1,MM7 |0012:260FE71C | MOVNTQ [ES:SI],MM3 |0016:0FD7CB | PMOVMSKB ECX,MM3 |0019:660FD7CB | PMOVMSKB ECX,XMM3 |001D:0F70CF02 | PSHUFW MM1,MM7,2 |0021:0F700D02 | PSHUFW MM1,[DI],2 |0025:0FC4D902 | PINSRW MM3,CX,2 |0029:0FC4D902 | PINSRW MM3,ECX,2 |002D:0FC41C02 | PINSRW MM3,[SI],2 |0031:660FC4D902 | PINSRW XMM3,CX,2 |0036:660FC4D902 | PINSRW XMM3,ECX,2 |003B:660FC41C02 | PINSRW XMM3,[SI],2 |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:0FF7CF | MASKMOVQ MM1,MM7 |00000003:0FF7CF | MASKMOVQ [EDI],MM1,MM7 |00000006:670FE71C | MOVNTQ [SI],MM3 |0000000A:0FE71E | MOVNTQ [ESI],MM3 |0000000D:0FD7CB | PMOVMSKB ECX,MM3 |00000010:660FD7CB | PMOVMSKB ECX,XMM3 |00000014:0F70CF02 | PSHUFW MM1,MM7,2 |00000018:0F704C9F1002 | PSHUFW MM1,[EDI+4*EBX+16],2 |0000001E:0FC4D902 | PINSRW MM3,CX,2 |00000022:0FC4D902 | PINSRW MM3,ECX,2 |00000026:670FC41C02 | PINSRW MM3,[SI],2 |0000002B:660FC4D902 | PINSRW XMM3,CX,2 |00000030:660FC4D902 | PINSRW XMM3,ECX,2 |00000035:66670FC41C02 | PINSRW XMM3,[SI],2 |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:0FF7CF | MASKMOVQ MM1,MM7 |00000003:0FF7CF | MASKMOVQ [RDI],MM1,MM7 |00000006:0FE71E | MOVNTQ [RSI],MM3 |00000009:670FE71E | MOVNTQ [ESI],MM3 |0000000D:0FD7CB | PMOVMSKB ECX,MM3 |00000010:440FD7FB | PMOVMSKB R15D,MM3 |00000014:660FD7CB | PMOVMSKB ECX,XMM3 |00000018:66440FD7FB | PMOVMSKB R15D,XMM3 |0000001D:0F70CF02 | PSHUFW MM1,MM7,2 |00000021:67420F704C8F1002 | PSHUFW MM1,[EDI+4*R9D+16],2 |00000029:0FC4D902 | PINSRW MM3,CX,2 |0000002D:0FC4D902 | PINSRW MM3,ECX,2 |00000031:0FC4D902 | PINSRW MM3,RCX,2 |00000035:650FC41E02 | PINSRW MM3,[GS:RSI],2 |0000003A:660FC4D902 | PINSRW XMM3,CX,2 |0000003F:660FC4D902 | PINSRW XMM3,ECX,2 |00000044:660FC4D902 | PINSRW XMM3,RCX,2 |00000049:660FC41E02 | PINSRW XMM3,[RSI],2 | |ENDPROGRAM t3645`

Expected messages t3645.out
  `I0180 Assembling source file "t3645.htm". I0270 Assembling source "t3645". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3645". "t3645.htm"{67} I0510 Assembling program pass 1. "t3645.htm"{67} I0530 Assembling program pass 2 - final. "t3645.htm"{67} I0660 16bit TINY BIN file "t3645.bin" created, size=206. "t3645.htm"{120} I0650 Program "t3645" assembled in 2 passes with errorlevel 0. "t3645.htm"{120} I0750 Source "t3645" (138 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3645.htm.lst" created, size=2937. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲