| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5442: Machine instructions VGATHERDPS VGATHERDPD VGATHERQPS VGATHERQPD

Tested procedures
  IizVGATHERDPS IizVGATHERDPD IizVGATHERQPS IizVGATHERQPD

Source & expected listing t5442.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,DUMPALL=OFF,CPU=X64,SIMD=AVX512,EVEX=ON,MVEX=ON | |t5442 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C4E261934C1540 | VGATHERQPS XMM1,[XMM2+RBP+40h],XMM3 |00000007:C4E265934C1540 | VGATHERQPS XMM1,[YMM2+RBP+40h],XMM3 |0000000E:62F27D0B934C1510<2 | VGATHERQPS XMM1,[XMM2+RBP+40h],MASK=K3 |00000016:62F27D2B934C1510<2 | VGATHERQPS XMM1,[YMM2+RBP+40h],MASK=K3 |0000001E:62F27D4B934C1510<2 | VGATHERQPS YMM1,[ZMM2+RBP+40h],MASK=K3 |00000026:C4E2E1934C1540 | VGATHERQPD XMM1,[XMM2+RBP+40h],XMM3 |0000002D:C4E2E5934C1540 | VGATHERQPD YMM1,[YMM2+RBP+40h],YMM3 |00000034:62F2FD0B934C1508<3 | VGATHERQPD XMM1,[XMM2+RBP+40h],MASK=K3 |0000003C:62F2FD2B934C1508<3 | VGATHERQPD YMM1,[YMM2+RBP+40h],MASK=K3 |00000044:62F2FD4B934C1508<3 | VGATHERQPD ZMM1,[ZMM2+RBP+40h],MASK=K3 |0000004C:C4E2E1924C1540 | VGATHERDPD XMM1,[XMM2+RBP+40h],XMM3 |00000053:C4E2E5924C1540 | VGATHERDPD YMM1,[XMM2+RBP+40h],YMM3 |0000005A:62F2FD0B924C1508<3 | VGATHERDPD XMM1,[XMM2+RBP+40h],MASK=K3 |00000062:62F2FD2B924C1508<3 | VGATHERDPD YMM1,[XMM2+RBP+40h],MASK=K3 |0000006A:62F2FD4B924C1508<3 | VGATHERDPD ZMM1,[YMM2+RBP+40h],MASK=K3 |00000072:62F2F90B924C1508<3 | VGATHERDPD ZMM1,[ZMM2+RBP+40h],MASK=K3 ; MVEX, no conversion. |0000007A:C4E261924C1540 | VGATHERDPS XMM1,[XMM2+RBP+40h],XMM3 |00000081:C4E265924C1540 | VGATHERDPS YMM1,[YMM2+RBP+40h],YMM3 |00000088:62F27D0B924C1510<2 | VGATHERDPS XMM1,[XMM2+RBP+40h],MASK=K3 |00000090:62F27D2B924C1510<2 | VGATHERDPS YMM1,[YMM2+RBP+40h],MASK=K3 |00000098:62F27D4B924C1510<2 | VGATHERDPS ZMM1,[ZMM2+RBP+40h],MASK=K3 |000000A0:62F2790B924C1510<2 | VGATHERDPS ZMM1,[ZMM2+RBP+40h],MASK=K3,PREFIX=MVEX,OPER=0 ; No conversion. |000000A8:62F2793B924C1520<1 | VGATHERDPS ZMM1,[ZMM2+RBP+40h],MASK=K3,PREFIX=MVEX,OPER=3 ; {float16}. |000000B0:62F2794B924C1540 | VGATHERDPS ZMM1,[ZMM2+RBP+40h],MASK=K3,PREFIX=MVEX,OPER=4 ; {uint8}. |000000B8:62F2795B924C1540 | VGATHERDPS ZMM1,[ZMM2+RBP+40h],MASK=K3,PREFIX=MVEX,OPER=5 ; {sint8}. |000000C0:62F2796B924C1520<1 | VGATHERDPS ZMM1,[ZMM2+RBP+40h],MASK=K3,PREFIX=MVEX,OPER=6 ; {uint16}. |000000C8:62F2797B924C1520<1 | VGATHERDPS ZMM1,[ZMM2+RBP+40h],MASK=K3,PREFIX=MVEX,OPER=7 ; {sint16}. | |ENDPROGRAM t5442`

Expected messages t5442.out
  `I0180 Assembling source file "t5442.htm". I0270 Assembling source "t5442". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5442". "t5442.htm"{58} I0510 Assembling program pass 1. "t5442.htm"{58} I0530 Assembling program pass 2 - final. "t5442.htm"{58} I0660 16bit TINY BIN file "t5442.bin" created, size=208. "t5442.htm"{87} I0650 Program "t5442" assembled in 2 passes with errorlevel 0. "t5442.htm"{87} I0750 Source "t5442" (105 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5442.htm.lst" created, size=2426. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲