| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t6124: Machine instructions VSUBRPS VADDSETSPS VPMADD233D

Tested procedures
  IiyVSUBRPS IiyVADDSETSPS IiyVPMADD233D

Source & expected listing t6124.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,MVEX=ON | |t6124 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F2690C6DCB | VSUBRPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=0 ; {dcba}. |00000006:62F2691C6DCB | VSUBRPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=1 ; {cdab}. |0000000C:62F2692C6DCB | VSUBRPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=2 ; {badc}. |00000012:62F2693C6DCB | VSUBRPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=3 ; {dacb}. |00000018:62F2694C6DCB | VSUBRPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=4 ; {aaaa}. |0000001E:62F2695C6DCB | VSUBRPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=5 ; {bbbb}. |00000024:62F2696C6DCB | VSUBRPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=6 ; {cccc}. |0000002A:62F2697C6DCB | VSUBRPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=7 ; {dddd}. |00000030:62F2699C6DCB | VSUBRPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=1,OPER=1 ; {rn}. |00000036:62F269BC6DCB | VSUBRPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=1,OPER=3 ; {rz}. |0000003C:62F269FC6DCB | VSUBRPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=1,OPER=7 ; {rz-sae}. |00000042:62F269FC6DCB | VSUBRPS ZMM1,ZMM2,ZMM3,MASK=K4,ROUND=ZERO,SAE=ON |00000048:62F2690C6D4D01<6 | VSUBRPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=0 ; {16to16}. |0000004F:62F2691C6D4D10<2 | VSUBRPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=1 ; {1to16}. |00000056:62F2692C6D4D04<4 | VSUBRPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=2 ; {4to16}. |0000005D:62F2693C6D4D02<5 | VSUBRPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=3 ; {float16}. |00000064:62F2694C6D4D04<4 | VSUBRPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=4 ; {uint8}. |0000006B:62F2696C6D4D02<5 | VSUBRPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=6 ; {uint16}. |00000072:62F2697C6D4D02<5 | VSUBRPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=7 ; {sint16}. |00000079:62F2690CCCCB | VADDSETSPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=0 ; {dcba}. |0000007F:62F2690CCC4D01<6 | VADDSETSPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=0 ; {16to16}. |00000086:62F2690CB4CB | VPMADD233D ZMM1,ZMM2,ZMM3,MASK=K4 |0000008C:62F2690CB4CB | VPMADD233D ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=0 ; No swizzle. |00000092:62F2690CB44D01<6 | VPMADD233D ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=0 ; {16to16}. |00000099:62F2698CB44D01<6 | VPMADD233D ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=0,EH=ON ; {16to16}. |000000A0:62F2692CB44D04<4 | VPMADD233D ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=2 ; {4to16}. |000000A7:62F269ACB44D04<4 | VPMADD233D ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=2,EH=ON ; {4to16}. | |ENDPROGRAM t6124`

Expected messages t6124.out
  `I0180 Assembling source file "t6124.htm". I0270 Assembling source "t6124". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t6124". "t6124.htm"{55} I0510 Assembling program pass 1. "t6124.htm"{55} I0530 Assembling program pass 2 - final. "t6124.htm"{55} I0660 16bit TINY BIN file "t6124.bin" created, size=174. "t6124.htm"{84} I0650 Program "t6124" assembled in 2 passes with errorlevel 0. "t6124.htm"{84} I0750 Source "t6124" (102 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t6124.htm.lst" created, size=2628. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲