| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3050: Machine instructions ROL ROLB ROLW ROLD in 16bit mode

Tested procedures
  IigROL IigROLB IigROLW IigROLD

Source & expected listing t3050.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=36,CPU=386 | |t3050 PROGRAM FORMAT=BIN,IMAGEBASE=0,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:D2C0 | ROL AL,CL |0002:D0C0 | ROL AL |0004:D0C0 | ROL AL,1 |0006:C0C001 | ROL AL,1,CODE=LONG |0009:C0C001 | ROL AL,1,IMM=BYTE |000C:C0C002 | ROL AL,2 |000F:D206[AE00] | ROL [MemByte],CL |0013:D006[AE00] | ROL [MemByte] |0017:D006[AE00] | ROL [MemByte],1 |001B:C006[AE00]01 | ROL [MemByte],1,CODE=LONG |0020:C006[AE00]01 | ROL [MemByte],1,IMM=BYTE |0025:C006[AE00]02 | ROL [MemByte],2 |002A:C00501 | ROL [DI],1,DATA=BYTE,IMM=BYTE |002D:67D007 | ROL [EDI],1,DATA=BYTE |0030:D3C0 | ROL AX,CL |0032:D1C0 | ROL AX |0034:D1C0 | ROL AX,1 |0036:C1C001 | ROL AX,1,CODE=LONG |0039:C1C001 | ROL AX,1,IMM=BYTE |003C:C1C002 | ROL AX,2 |003F:D306[AC00] | ROL [MemWord],CL |0043:D106[AC00] | ROL [MemWord] |0047:D106[AC00] | ROL [MemWord],1 |004B:C106[AC00]01 | ROL [MemWord],1,CODE=LONG |0050:C106[AC00]01 | ROL [MemWord],1,IMM=BYTE |0055:C106[AC00]02 | ROL [MemWord],2 |005A:C10501 | ROL [DI],1,DATA=WORD,IMM=BYTE |005D:67D107 | ROL [EDI],1,DATA=WORD |0060:66D3C0 | ROL EAX,CL |0063:66D1C0 | ROL EAX |0066:66D1C0 | ROL EAX,1 |0069:66C1C001 | ROL EAX,1,CODE=LONG |006D:66C1C001 | ROL EAX,1,IMM=BYTE |0071:66C1C002 | ROL EAX,2 |0075:66D306[A800] | ROL [MemDword],CL |007A:66D106[A800] | ROL [MemDword] |007F:66D106[A800] | ROL [MemDword],1 |0084:66C106[A800]01 | ROL [MemDword],1,CODE=LONG |008A:66C106[A800]01 | ROL [MemDword],1,IMM=BYTE |0090:66C106[A800]02 | ROL [MemDword],2 |0096:66C10501 | ROL [DI],1,DATA=DWORD,IMM=BYTE |009A:6667D107 | ROL [EDI],1,DATA=DWORD |009E:D205 | ROLB [DI],CL |00A0:D305 | ROLW [DI],CL |00A2:66D305 | ROLD [DI],CL |00A5:9087C9 | ALIGN QWORD |00A8:00000000 |MemDword D D |00AC:0000 |MemWord D W |00AE:00 |MemByte D B | |ENDPROGRAM t3050`

Expected messages t3050.out
  `I0180 Assembling source file "t3050.htm". I0270 Assembling source "t3050". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3050". "t3050.htm"{58} I0510 Assembling program pass 1. "t3050.htm"{58} I0510 Assembling program pass 2. "t3050.htm"{58} I0510 Assembling program pass 3. "t3050.htm"{58} I0530 Assembling program pass 4 - final. "t3050.htm"{58} I0660 16bit TINY BIN file "t3050.bin" created, size=175. "t3050.htm"{109} I0650 Program "t3050" assembled in 4 passes with errorlevel 0. "t3050.htm"{109} I0750 Source "t3050" (129 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3050.htm.lst" created, size=2992. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲