| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t4580: Machine instructions VPCOMUD VPCOMLTUD VPCOMLEUD VPCOMGTUD VPCOMGEUD VPCOMEQUD VPCOMNEQUD VPCOMFALSEUD VPCOMTRUEUD

Tested procedures
  IixVPCOMUD IixVPCOMLTUD IixVPCOMLEUD IixVPCOMGTUD IixVPCOMGEUD IixVPCOMEQUD IixVPCOMNEQUD IixVPCOMFALSEUD IixVPCOMTRUEUD

Source & expected listing t4580.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=24,CPU=X64,SIMD=AVX,AMD=ON,XOP=ON,PROT=ON | |t4580 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:8FE868EECB04 | VPCOMUD XMM1,XMM2,XMM3,4 |00000006:8FE868EECB00 | VPCOMLTUD XMM1,XMM2,XMM3 |0000000C:8FE868EECB01 | VPCOMLEUD XMM1,XMM2,XMM3 |00000012:8FE868EECB02 | VPCOMGTUD XMM1,XMM2,XMM3 |00000018:8FE868EECB03 | VPCOMGEUD XMM1,XMM2,XMM3 |0000001E:8FE868EECB04 | VPCOMEQUD XMM1,XMM2,XMM3 |00000024:8FE868EECB05 | VPCOMNEQUD XMM1,XMM2,XMM3 |0000002A:8FE868EECB06 | VPCOMFALSEUD XMM1,XMM2,XMM3 |00000030:8FE868EECB07 | VPCOMTRUEUD XMM1,XMM2,XMM3 |00000036:8FE868EE0E04 | VPCOMUD XMM1,XMM2,[RSI],4 |0000003C:8FE868EE0E00 | VPCOMLTUD XMM1,XMM2,[RSI] |00000042:8FE868EE0E01 | VPCOMLEUD XMM1,XMM2,[RSI] |00000048:8FE868EE0E02 | VPCOMGTUD XMM1,XMM2,[RSI] |0000004E:8FE868EE0E03 | VPCOMGEUD XMM1,XMM2,[RSI] |00000054:8FE868EE0E04 | VPCOMEQUD XMM1,XMM2,[RSI] |0000005A:8FE868EE0E05 | VPCOMNEQUD XMM1,XMM2,[RSI] |00000060:8FE868EE0E06 | VPCOMFALSEUD XMM1,XMM2,[RSI] |00000066:8FE868EE0E07 | VPCOMTRUEUD XMM1,XMM2,[RSI] | |ENDPROGRAM t4580`

Expected messages t4580.out
  `I0180 Assembling source file "t4580.htm". I0270 Assembling source "t4580". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t4580". "t4580.htm"{73} I0510 Assembling program pass 1. "t4580.htm"{73} I0530 Assembling program pass 2 - final. "t4580.htm"{73} I0660 16bit TINY BIN file "t4580.bin" created, size=108. "t4580.htm"{93} I0650 Program "t4580" assembled in 2 passes with errorlevel 0. "t4580.htm"{93} I0750 Source "t4580" (111 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t4580.htm.lst" created, size=1275. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲