| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3272: Machine instructions IMUL IMULB IMULW IMULD in 32bit mode

Tested procedures
  IigIMUL IigIMULB IigIMULW IigIMULD

Source & expected listing t3272.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=32, CPU=386 | |t3272 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:F6E9 | IMUL CL |00000002:66F7E9 | IMUL CX |00000005:F7E9 | IMUL ECX |00000007:F62D[7E000000] | IMUL [MemByte] |0000000D:66F72D[7C000000] | IMUL [MemWord] |00000014:F72D[78000000] | IMUL [MemDword] |0000001A:F62E | IMUL [ESI],DATA=BYTE |0000001C:F62E | IMULB [ESI] |0000001E:66F72E | IMUL [ESI],DATA=WORD |00000021:66F72E | IMULW [ESI] |00000024:F72E | IMUL [ESI],DATA=DWORD |00000026:F72E | IMULD [ESI] |00000028:660FAFCA | IMUL CX,DX |0000002C:0FAFCA | IMUL ECX,EDX |0000002F:660FAF0E | IMUL CX,[ESI] |00000033:0FAF0E | IMUL ECX,[ESI] |00000036:69CA7EFFFFFF | IMUL ECX,EDX,-130 |0000003C:69CA7FFFFFFF | IMUL ECX,EDX,-129 |00000042:6BCA80 | IMUL ECX,EDX,-128,IMM=BYTE |00000045:6BCA81 | IMUL ECX,EDX,-127,IMM=BYTE |00000048:6BCA7E | IMUL ECX,EDX,+126,IMM=BYTE |0000004B:6BCA7F | IMUL ECX,EDX,+127,IMM=BYTE |0000004E:69CA80000000 | IMUL ECX,EDX,+128 |00000054:69CA81000000 | IMUL ECX,EDX,+129 |0000005A:66690E0300 | IMUL CX,[ESI],3 |0000005F:666B0E03 | IMUL CX,[ESI],3,IMM=BYTE |00000063:66690E0300 | IMUL CX,[ESI],3,IMM=WORD |00000068:690E03000000 | IMUL ECX,[ESI],3 |0000006E:6B0E03 | IMUL ECX,[ESI],3,IMM=BYTE |00000071:690E03000000 | IMUL ECX,[ESI],3,IMM=DWORD |00000077:90 | ALIGN QWORD |00000078:00000000 |MemDword DD D |0000007C:0000 |MemWord DW W |0000007E:00 |MemByte DB B | | ENDPROGRAM t3272`

Expected messages t3272.out
  `I0180 Assembling source file "t3272.htm". I0270 Assembling source "t3272". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3272". "t3272.htm"{58} I0510 Assembling program pass 1. "t3272.htm"{58} I0510 Assembling program pass 2. "t3272.htm"{58} I0510 Assembling program pass 3. "t3272.htm"{58} I0530 Assembling program pass 4 - final. "t3272.htm"{58} I0660 16bit TINY BIN file "t3272.bin" created, size=127. "t3272.htm"{94} I0650 Program "t3272" assembled in 4 passes with errorlevel 0. "t3272.htm"{94} I0750 Source "t3272" (114 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3272.htm.lst" created, size=2042. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲