| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t6120: Machine instructions VPADCD VPSBBD VPADDSETCD VPSUBSETBD VPSUBSETBD

Tested procedures
  IiyVPADCD IiyVPSBBD IiyVPADDSETCD IiyVPSUBSETBD IiyVPSUBRSETBD

Source & expected listing t6120.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,MVEX=ON | |t6120 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F2690C5CCB | VPADCD ZMM1,K2,ZMM3,MASK=K4,EH=0,OPER=0 ; {dcba}. |00000006:62F2691C5CCB | VPADCD ZMM1,K2,ZMM3,MASK=K4,EH=0,OPER=1 ; {cdab}. |0000000C:62F2692C5CCB | VPADCD ZMM1,K2,ZMM3,MASK=K4,EH=0,OPER=2 ; {badc}. |00000012:62F2693C5CCB | VPADCD ZMM1,K2,ZMM3,MASK=K4,EH=0,OPER=3 ; {dacb}. |00000018:62F2694C5CCB | VPADCD ZMM1,K2,ZMM3,MASK=K4,EH=0,OPER=4 ; {aaaa}. |0000001E:62F2695C5CCB | VPADCD ZMM1,K2,ZMM3,MASK=K4,EH=0,OPER=5 ; {bbbb}. |00000024:62F2696C5CCB | VPADCD ZMM1,K2,ZMM3,MASK=K4,EH=0,OPER=6 ; {cccc}. |0000002A:62F2697C5CCB | VPADCD ZMM1,K2,ZMM3,MASK=K4,EH=0,OPER=7 ; {dddd}. |00000030:62F2690C5C4D01<6 | VPADCD ZMM1,K2,[RBP+40h],MASK=K4,OPER=0 ; {16to16}. |00000037:62F2691C5C4D10<2 | VPADCD ZMM1,K2,[RBP+40h],MASK=K4,OPER=1 ; {1to16}. |0000003E:62F2692C5C4D04<4 | VPADCD ZMM1,K2,[RBP+40h],MASK=K4,OPER=2 ; {4to16}. |00000045:62F2694C5C4D04<4 | VPADCD ZMM1,K2,[RBP+40h],MASK=K4,OPER=4 ; {uint8}. |0000004C:62F2695C5C4D04<4 | VPADCD ZMM1,K2,[RBP+40h],MASK=K4,OPER=5 ; {sint8}. |00000053:62F2696C5C4D02<5 | VPADCD ZMM1,K2,[RBP+40h],MASK=K4,OPER=6 ; {uint16}. |0000005A:62F2697C5C4D02<5 | VPADCD ZMM1,K2,[RBP+40h],MASK=K4,OPER=7 ; {sint16}. |00000061:62F2690C5ECB | VPSBBD ZMM1,K2,ZMM3,MASK=K4,EH=0,OPER=0 ; {dcba}. |00000067:62F2690C5E4D01<6 | VPSBBD ZMM1,K2,[RBP+40h],MASK=K4,OPER=0 ; {16to16}. |0000006E:62F2690C5DCB | VPADDSETCD ZMM1,K2,ZMM3,MASK=K4,EH=0,OPER=0 ; {dcba}. |00000074:62F2690C5D4D01<6 | VPADDSETCD ZMM1,K2,[RBP+40h],MASK=K4,OPER=0 ; {16to16}. |0000007B:62F2690C5FCB | VPSUBSETBD ZMM1,K2,ZMM3,MASK=K4,EH=0,OPER=0 ; {dcba}. |00000081:62F2690C5F4D01<6 | VPSUBSETBD ZMM1,K2,[RBP+40h],MASK=K4,OPER=0 ; {16to16}. |00000088:62F2690C6FCB | VPSUBRSETBD ZMM1,K2,ZMM3,MASK=K4,EH=0,OPER=0 ; {dcba}. |0000008E:62F2690C6F4D01<6 | VPSUBRSETBD ZMM1,K2,[RBP+40h],MASK=K4,OPER=0 ; {16to16}. | |ENDPROGRAM t6120`

Expected messages t6120.out
  `I0180 Assembling source file "t6120.htm". I0270 Assembling source "t6120". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t6120". "t6120.htm"{61} I0510 Assembling program pass 1. "t6120.htm"{61} I0530 Assembling program pass 2 - final. "t6120.htm"{61} I0660 16bit TINY BIN file "t6120.bin" created, size=149. "t6120.htm"{86} I0650 Program "t6120" assembled in 2 passes with errorlevel 0. "t6120.htm"{86} I0750 Source "t6120" (104 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t6120.htm.lst" created, size=2235. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲