| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3073: Machine instructions RCR RCRB RCRW RCRD RCRQ in 64bit mode

Tested procedures
  IigRCR IigRCRB IigRCRW IigRCRD IigRCRQ

Source & expected listing t3073.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=36,CPU=X64 | |t3073 PROGRAM FORMAT=BIN,IMAGEBASE=0,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:D2D8 | RCR AL,CL |00000002:D0D8 | RCR AL |00000004:D0D8 | RCR AL,1 |00000006:C0D801 | RCR AL,1,CODE=LONG |00000009:C0D801 | RCR AL,1,IMM=BYTE |0000000C:C0D802 | RCR AL,2 |0000000F:D21D19010000 | RCR [MemByte],CL |00000015:D01D13010000 | RCR [MemByte] |0000001B:D01D0D010000 | RCR [MemByte],1 |00000021:C01D0601000001 | RCR [MemByte],1,CODE=LONG |00000028:C01DFF00000001 | RCR [MemByte],1,IMM=BYTE |0000002F:C01DF800000002 | RCR [MemByte],2 |00000036:C01F01 | RCR [RDI],1,DATA=BYTE,IMM=BYTE |00000039:67D01F | RCR [EDI],1,DATA=BYTE |0000003C:66D3D8 | RCR AX,CL |0000003F:66D1D8 | RCR AX |00000042:66D1D8 | RCR AX,1 |00000045:66C1D801 | RCR AX,1,CODE=LONG |00000049:66C1D801 | RCR AX,1,IMM=BYTE |0000004D:66C1D802 | RCR AX,2 |00000051:66D31DD4000000 | RCR [MemWord],CL |00000058:66D11DCD000000 | RCR [MemWord] |0000005F:66D11DC6000000 | RCR [MemWord],1 |00000066:66C11DBE00000001 | RCR [MemWord],1,CODE=LONG |0000006E:66C11DB600000001 | RCR [MemWord],1,IMM=BYTE |00000076:66C11DAE00000002 | RCR [MemWord],2 |0000007E:66C11F01 | RCR [RDI],1,DATA=WORD,IMM=BYTE |00000082:6667D11F | RCR [EDI],1,DATA=WORD |00000086:D3D8 | RCR EAX,CL |00000088:D1D8 | RCR EAX |0000008A:D1D8 | RCR EAX,1 |0000008C:C1D801 | RCR EAX,1,CODE=LONG |0000008F:C1D801 | RCR EAX,1,IMM=BYTE |00000092:C1D802 | RCR EAX,2 |00000095:D31D8D000000 | RCR [MemDword],CL |0000009B:D11D87000000 | RCR [MemDword] |000000A1:D11D81000000 | RCR [MemDword],1 |000000A7:C11D7A00000001 | RCR [MemDword],1,CODE=LONG |000000AE:C11D7300000001 | RCR [MemDword],1,IMM=BYTE |000000B5:C11D6C00000002 | RCR [MemDword],2 |000000BC:67C11F01 | RCR [EDI],1,DATA=DWORD,IMM=BYTE |000000C0:D11F | RCR [RDI],1,DATA=DWORD |000000C2:48D3D8 | RCR RAX,CL |000000C5:48D1D8 | RCR RAX |000000C8:48D1D8 | RCR RAX,1 |000000CB:48C1D801 | RCR RAX,1,CODE=LONG |000000CF:48C1D801 | RCR RAX,1,IMM=BYTE |000000D3:48C1D802 | RCR RAX,2 |000000D7:48D31D42000000 | RCR [MemQword],CL |000000DE:48D11D3B000000 | RCR [MemQword] |000000E5:48D11D34000000 | RCR [MemQword],1 |000000EC:48C11D2C00000001 | RCR [MemQword],1,CODE=LONG |000000F4:48C11D2400000001 | RCR [MemQword],1,IMM=BYTE |000000FC:48C11D1C00000002 | RCR [MemQword],2 |00000104:6741C11801 | RCR [R8D],1,DATA=DWORD,IMM=BYTE |00000109:41D11C24 | RCR [R12],1,DATA=DWORD |0000010D:4AD15CA500 | RCR [RBP+4*R12],1,DATA=QWORD |00000112:D21F | RCRB [RDI],CL |00000114:66D31F | RCRW [RDI],CL |00000117:D31F | RCRD [RDI],CL |00000119:48D31F | RCRQ [RDI],CL |0000011C:0F1F4000 | ALIGN QWORD |00000120:0000000000000000 |MemQword D Q |00000128:00000000 |MemDword D D |0000012C:0000 |MemWord D W |0000012E:00 |MemByte D B | |ENDPROGRAM t3073`

Expected messages t3073.out
  `I0180 Assembling source file "t3073.htm". I0270 Assembling source "t3073". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3073". "t3073.htm"{61} I0510 Assembling program pass 1. "t3073.htm"{61} I0510 Assembling program pass 2. "t3073.htm"{61} I0510 Assembling program pass 3. "t3073.htm"{61} I0530 Assembling program pass 4 - final. "t3073.htm"{61} I0660 16bit TINY BIN file "t3073.bin" created, size=303. "t3073.htm"{129} I0650 Program "t3073" assembled in 4 passes with errorlevel 0. "t3073.htm"{129} I0750 Source "t3073" (149 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3073.htm.lst" created, size=3952. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲