| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3051: Machine instructions ROR RORB RORW RORD in 16bit mode

Tested procedures
  IigROR IigRORB IigRORW IigRORD

Source & expected listing t3051.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=36,CPU=386 | |t3051 PROGRAM FORMAT=BIN,IMAGEBASE=0,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:D2C8 | ROR AL,CL |0002:D0C8 | ROR AL |0004:D0C8 | ROR AL,1 |0006:C0C801 | ROR AL,1,CODE=LONG |0009:C0C801 | ROR AL,1,IMM=BYTE |000C:C0C802 | ROR AL,2 |000F:D20E[AE00] | ROR [MemByte],CL |0013:D00E[AE00] | ROR [MemByte] |0017:D00E[AE00] | ROR [MemByte],1 |001B:C00E[AE00]01 | ROR [MemByte],1,CODE=LONG |0020:C00E[AE00]01 | ROR [MemByte],1,IMM=BYTE |0025:C00E[AE00]02 | ROR [MemByte],2 |002A:C00D01 | ROR [DI],1,DATA=BYTE,IMM=BYTE |002D:67D00F | ROR [EDI],1,DATA=BYTE |0030:D3C8 | ROR AX,CL |0032:D1C8 | ROR AX |0034:D1C8 | ROR AX,1 |0036:C1C801 | ROR AX,1,CODE=LONG |0039:C1C801 | ROR AX,1,IMM=BYTE |003C:C1C802 | ROR AX,2 |003F:D30E[AC00] | ROR [MemWord],CL |0043:D10E[AC00] | ROR [MemWord] |0047:D10E[AC00] | ROR [MemWord],1 |004B:C10E[AC00]01 | ROR [MemWord],1,CODE=LONG |0050:C10E[AC00]01 | ROR [MemWord],1,IMM=BYTE |0055:C10E[AC00]02 | ROR [MemWord],2 |005A:C10D01 | ROR [DI],1,DATA=WORD,IMM=BYTE |005D:67D10F | ROR [EDI],1,DATA=WORD |0060:66D3C8 | ROR EAX,CL |0063:66D1C8 | ROR EAX |0066:66D1C8 | ROR EAX,1 |0069:66C1C801 | ROR EAX,1,CODE=LONG |006D:66C1C801 | ROR EAX,1,IMM=BYTE |0071:66C1C802 | ROR EAX,2 |0075:66D30E[A800] | ROR [MemDword],CL |007A:66D10E[A800] | ROR [MemDword] |007F:66D10E[A800] | ROR [MemDword],1 |0084:66C10E[A800]01 | ROR [MemDword],1,CODE=LONG |008A:66C10E[A800]01 | ROR [MemDword],1,IMM=BYTE |0090:66C10E[A800]02 | ROR [MemDword],2 |0096:66C10D01 | ROR [DI],1,DATA=DWORD,IMM=BYTE |009A:6667D10F | ROR [EDI],1,DATA=DWORD |009E:D20D | RORB [DI],CL |00A0:D30D | RORW [DI],CL |00A2:66D30D | RORD [DI],CL |00A5:9087C9 | ALIGN QWORD |00A8:00000000 |MemDword D D |00AC:0000 |MemWord D W |00AE:00 |MemByte D B | |ENDPROGRAM t3051`

Expected messages t3051.out
  `I0180 Assembling source file "t3051.htm". I0270 Assembling source "t3051". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3051". "t3051.htm"{58} I0510 Assembling program pass 1. "t3051.htm"{58} I0510 Assembling program pass 2. "t3051.htm"{58} I0510 Assembling program pass 3. "t3051.htm"{58} I0530 Assembling program pass 4 - final. "t3051.htm"{58} I0660 16bit TINY BIN file "t3051.bin" created, size=175. "t3051.htm"{109} I0650 Program "t3051" assembled in 4 passes with errorlevel 0. "t3051.htm"{109} I0750 Source "t3051" (129 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3051.htm.lst" created, size=2992. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲