| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3041: Machine instructions MOV MOVB MOVW MOVD MOVQ in 16bit mode

Tested procedures
  IigMOV IigMOVB IigMOVW IigMOVD IigMOVQ

Source & expected listing t3041.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=34,DUMPALL=OFF,CPU=386 | |t3041 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:88D1 | MOV CL,DL |0002:8ACA | MOV CL,DL,CODE=LONG |0004:8A0C | MOV CL,[SI] |0006:A0[2E01] | MOV AL,[MemByte] |0009:8A06[2E01] | MOV AL,[MemByte],CODE=LONG |000D:8A0E[2E01] | MOV CL,[MemByte] |0011:8815 | MOV [DI],DL |0013:A2[2E01] | MOV [MemByte],AL |0016:8806[2E01] | MOV [MemByte],AL,CODE=LONG |001A:8816[2E01] | MOV [MemByte],DL |001E:89D1 | MOV CX,DX |0020:8BCA | MOV CX,DX,CODE=LONG |0022:8B0C | MOV CX,[SI] |0024:A1[2C01] | MOV AX,[MemWord] |0027:8B06[2C01] | MOV AX,[MemWord],CODE=LONG |002B:8B0E[2C01] | MOV CX,[MemWord] |002F:8915 | MOV [DI],DX |0031:A3[2C01] | MOV [MemWord],AX |0034:8906[2C01] | MOV [MemWord],AX,CODE=LONG |0038:8916[2C01] | MOV [MemWord],DX |003C:6689D1 | MOV ECX,EDX |003F:668BCA | MOV ECX,EDX,CODE=LONG |0042:668B0C | MOV ECX,[SI] |0045:66A1[2801] | MOV EAX,[MemDword] |0049:668B06[2801] | MOV EAX,[MemDword],CODE=LONG |004E:668B0E[2801] | MOV ECX,[MemDword] |0053:668915 | MOV [DI],EDX |0056:66A3[2801] | MOV [MemDword],EAX |005A:668906[2801] | MOV [MemDword],EAX,CODE=LONG |005F:668916[2801] | MOV [MemDword],EDX |0064:8EC2 | MOV ES,DX |0066:8EC2 | MOV ES,EDX |0068:8E04 | MOV ES,[SI] |006A:8E06[2C01] | MOV ES,[MemWord] |006E:8CC9 | MOV CX,CS |0070:668CC9 | MOV ECX,CS |0073:8C0D | MOV [DI],CS |0075:8C0D | MOVW [DI],CS |0077:668C0D | MOVD [DI],CS |007A:8C0E[2C01] | MOV [MemWord],CS |007E:668C0E[2801] | MOV [MemDword],CS |0083:B102 | MOV CL,2 |0085:C6C102 | MOV CL,2,CODE=LONG |0088:B90200 | MOV CX,2 |008B:C7C10200 | MOV CX,2,CODE=LONG |008F:66B902000000 | MOV ECX,2 |0095:66C7C102000000 | MOV ECX,2,CODE=LONG |009C:C60502 | MOVB [DI],2 |009F:C7050200 | MOVW [DI],2 |00A3:66C70502000000 | MOVD [DI],2 |00AA:C606[2E01]02 | MOV [MemByte],2 |00AF:C706[2C01]0200 | MOV [MemWord],2 |00B5:66C706[2801]02000000 | MOV [MemDword],2 | | EUROASM MMX=ON |00BE:0F6ECA | MOVD MM1,EDX |00C1:0F7ED1 | MOVD ECX,MM2 |00C4:0F6E0C | MOVD MM1,[SI] |00C7:0F6E0E[2801] | MOVD MM1,[MemDword] |00CC:0F7E15 | MOVD [DI],MM2 |00CF:0F7E16[2801] | MOVD [MemDword],MM2 |00D4:0F6FCA | MOVQ MM1,MM2 |00D7:0F7FD1 | MOVQ MM1,MM2,CODE=LONG |00DA:670F6F0E | MOVQ MM1,[ESI] |00DE:0F7F15 | MOVQ [DI],MM2 | | EUROASM SIMD=SSE |00E1:F30F7ECA | MOVQ XMM1,XMM2 |00E5:660FD6D1 | MOVQ XMM1,XMM2,CODE=LONG |00E9:660F6ECA | MOVD XMM1,EDX |00ED:660F7ED1 | MOVD ECX,XMM2 |00F1:660F6E0C | MOVD XMM1,[SI] |00F5:66670F7E17 | MOVD [EDI],XMM2 |00FA:F30F7ECA | MOVQ XMM1,XMM2 |00FE:660FD6D1 | MOVQ XMM1,XMM2,CODE=LONG |0102:F30F7E0C | MOVQ XMM1,[SI] |0106:660FD615 | MOVQ [DI],XMM2 | | EUROASM PRIV=ON |010A:0F21D1 | MOV ECX,DR2 |010D:0F23CA | MOV DR1,EDX |0110:0F20D1 | MOV ECX,CR2 | | EUROASM CPU=X64, AMD=ON |0113:F00F20C1 | MOV ECX,CR8 |0117:0F22C2 | MOV CR0,EDX |011A:F00F22C2 | MOV CR8,EDX | | EUROASM UNDOC=ON |011E:0F24D1 | MOV ECX,TR2 |0121:0F26CA | MOV TR1,EDX |0124:670F1F00 | ALIGN QWORD |0128:00000000 |MemDword D D |012C:0000 |MemWord D W |012E:00 |MemByte D B | |ENDPROGRAM t3041`

Expected messages t3041.out
  `I0180 Assembling source file "t3041.htm". I0270 Assembling source "t3041". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3041". "t3041.htm"{61} I0510 Assembling program pass 1. "t3041.htm"{61} I0510 Assembling program pass 2. "t3041.htm"{61} I0510 Assembling program pass 3. "t3041.htm"{61} I0530 Assembling program pass 4 - final. "t3041.htm"{61} I0660 16bit TINY BIN file "t3041.bin" created, size=303. "t3041.htm"{153} I0650 Program "t3041" assembled in 4 passes with errorlevel 0. "t3041.htm"{153} I0750 Source "t3041" (173 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3041.htm.lst" created, size=4971. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲