| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3325: Machine instructions INT INT1 INT3 INTO ICEBP SMI

Tested procedures
  IigINT IigINT1 IigINT3 IigINTO IigICEBP IigSMI

Source & expected listing t3325.htm.lst
  `| |EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=24, CPU=X64, UNDOC=ENABLE | |t3325 PROGRAM FORMAT=BIN,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:CD00 | INT 0 |0002:CD01 | INT 1 |0004:CD02 | INT 2 |0006:CD03 | INT 3 |0008:CD04 | INT 4 |000A:CD05 | INT 5 |000C:CDFF | INT 255 |000E:F1 | INT1 |000F:CC | INT3 |0010:CE | INTO |0011:F1 | ICEBP |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:CD00 | INT 0 |00000002:CD01 | INT 1 |00000004:CD02 | INT 2 |00000006:CD03 | INT 3 |00000008:CD04 | INT 4 |0000000A:CD05 | INT 5 |0000000C:CDFF | INT 255 |0000000E:F1 | INT1 |0000000F:F1 | ICEBP | | EUROASM AMD=ENABLED |00000010:F1 | SMI |00000011:CC | INT3 |00000012:CE | INTO |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:CD00 | INT 0 |00000002:CD01 | INT 1 |00000004:CD02 | INT 2 |00000006:CD03 | INT 3 |00000008:CD04 | INT 4 |0000000A:CD05 | INT 5 |0000000C:CDFF | INT 255 |0000000E:F1 | INT1 |0000000F:CC | INT3 | |ENDPROGRAM t3325`

Expected messages t3325.out
  `I0180 Assembling source file "t3325.htm". I0270 Assembling source "t3325". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3325". "t3325.htm"{64} I0510 Assembling program pass 1. "t3325.htm"{64} I0530 Assembling program pass 2 - final. "t3325.htm"{64} I0660 16bit TINY BIN file "t3325.bin" created, size=80. "t3325.htm"{101} I0650 Program "t3325" assembled in 2 passes with errorlevel 0. "t3325.htm"{101} I0750 Source "t3325" (119 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3325.htm.lst" created, size=1465. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲