| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3055: Machine instructions SHR SHRB SHRW SHRD in 16bit mode

Tested procedures
  IigSHR IigSHRB IigSHRW IigSHRD

Source & expected listing t3055.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=36,CPU=386 | |t3055 PROGRAM FORMAT=BIN,IMAGEBASE=0,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:D2E8 | SHR AL,CL |0002:D0E8 | SHR AL |0004:D0E8 | SHR AL,1 |0006:C0E801 | SHR AL,1,CODE=LONG |0009:C0E801 | SHR AL,1,IMM=BYTE |000C:C0E802 | SHR AL,2 |000F:D22E[2601] | SHR [MemByte],CL |0013:D02E[2601] | SHR [MemByte] |0017:D02E[2601] | SHR [MemByte],1 |001B:C02E[2601]01 | SHR [MemByte],1,CODE=LONG |0020:C02E[2601]01 | SHR [MemByte],1,IMM=BYTE |0025:C02E[2601]02 | SHR [MemByte],2 |002A:C02D01 | SHR [DI],1,DATA=BYTE,IMM=BYTE |002D:67D02F | SHR [EDI],1,DATA=BYTE |0030:D3E8 | SHR AX,CL |0032:D1E8 | SHR AX |0034:D1E8 | SHR AX,1 |0036:C1E801 | SHR AX,1,CODE=LONG |0039:C1E801 | SHR AX,1,IMM=BYTE |003C:C1E802 | SHR AX,2 |003F:D32E[2401] | SHR [MemWord],CL |0043:D12E[2401] | SHR [MemWord] |0047:D12E[2401] | SHR [MemWord],1 |004B:C12E[2401]01 | SHR [MemWord],1,CODE=LONG |0050:C12E[2401]01 | SHR [MemWord],1,IMM=BYTE |0055:C12E[2401]02 | SHR [MemWord],2 |005A:C12D01 | SHR [DI],1,DATA=WORD,IMM=BYTE |005D:67D12F | SHR [EDI],1,DATA=WORD |0060:66D3E8 | SHR EAX,CL |0063:66D1E8 | SHR EAX |0066:66D1E8 | SHR EAX,1 |0069:66C1E801 | SHR EAX,1,CODE=LONG |006D:66C1E801 | SHR EAX,1,IMM=BYTE |0071:66C1E802 | SHR EAX,2 |0075:66D32E[2001] | SHR [MemDword],CL |007A:66D12E[2001] | SHR [MemDword] |007F:66D12E[2001] | SHR [MemDword],1 |0084:66C12E[2001]01 | SHR [MemDword],1,CODE=LONG |008A:66C12E[2001]01 | SHR [MemDword],1,IMM=BYTE |0090:66C12E[2001]02 | SHR [MemDword],2 |0096:66C12D01 | SHR [DI],1,DATA=DWORD,IMM=BYTE |009A:6667D12F | SHR [EDI],1,DATA=DWORD |009E:D22D | SHRB [DI],CL |00A0:D32D | SHRW [DI],CL |00A2:66D32D | SHRD [DI],CL |00A5:66D3E8 | SHRD EAX,CL |00A8:66D1E8 | SHRD EAX |00AB:66D1E8 | SHRD EAX,1 |00AE:66C1E801 | SHRD EAX,1,IMM=BYTE |00B2:66C1E802 | SHRD EAX,2 |00B6: | ; Following instructions are double precision shift. |00B6:0FADD0 | SHRD AX,DX,CL |00B9:0FACD001 | SHRD AX,DX |00BD:0FACD001 | SHRD AX,DX,1 |00C1:0FACD002 | SHRD AX,DX,2 |00C5:0FAD16[2401] | SHRD [MemWord],DX,CL |00CA:0FAC16[2401]01 | SHRD [MemWord],DX |00D0:0FAC16[2401]01 | SHRD [MemWord],DX,1 |00D6:0FAC16[2401]03 | SHRD [MemWord],DX,3 |00DC:0FAD15 | SHRD [DI],DX,CL |00DF:0FAC1503 | SHRD [DI],DX,3 |00E3:660FADD0 | SHRD EAX,EDX,CL |00E7:660FACD001 | SHRD EAX,EDX |00EC:660FACD001 | SHRD EAX,EDX,1 |00F1:660FACD002 | SHRD EAX,EDX,2 |00F6:660FAD16[2001] | SHRD [MemDword],EDX,CL |00FC:660FAC16[2001]01 | SHRD [MemDword],EDX |0103:660FAC16[2001]01 | SHRD [MemDword],EDX,1 |010A:660FAC16[2001]02 | SHRD [MemDword],EDX,2 |0111:660FAD15 | SHRD [DI],EDX,CL |0115:660FAC1503 | SHRD [DI],EDX,3 |011A:87C987D287DB | ALIGN QWORD |0120:00000000 |MemDword D D |0124:0000 |MemWord D W |0126:00 |MemByte D B | |ENDPROGRAM t3055`

Expected messages t3055.out
  `I0180 Assembling source file "t3055.htm". I0270 Assembling source "t3055". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3055". "t3055.htm"{58} I0510 Assembling program pass 1. "t3055.htm"{58} I0510 Assembling program pass 2. "t3055.htm"{58} I0510 Assembling program pass 3. "t3055.htm"{58} I0530 Assembling program pass 4 - final. "t3055.htm"{58} I0660 16bit TINY BIN file "t3055.bin" created, size=295. "t3055.htm"{135} I0650 Program "t3055" assembled in 4 passes with errorlevel 0. "t3055.htm"{135} I0750 Source "t3055" (155 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3055.htm.lst" created, size=4436. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲