| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5660: Machine instructions VRCP28SS VRCP28SD VRCP28PS VRCP28PD

Tested procedures
  IiyVRCP28SS IiyVRCP28SD IiyVRCP28PS IiyVRCP28PD

Source & expected listing t5660.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON | |t5660 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F26D08CBCB | VRCP28SS XMM1,XMM2,XMM3 |00000006:62F26D9CCBCB | VRCP28SS XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON,SAE=ON |0000000C:62F26D08CB4D10<2 | VRCP28SS XMM1,XMM2,[RBP+40h] |00000013:62F26D8CCB4D10<2 | VRCP28SS XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |0000001A:62F2ED08CBCB | VRCP28SD XMM1,XMM2,XMM3 |00000020:62F2ED8CCBCB | VRCP28SD XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000026:62F2ED08CB4D08<3 | VRCP28SD XMM1,XMM2,[RBP+40h] |0000002D:62F2ED8CCB4D08<3 | VRCP28SD XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000034:62F27DDBCACA | VRCP28PS ZMM1,ZMM2,MASK=K3,ZEROING=ON,SAE=ON |0000003A:62F27DCBCA4D01<6 | VRCP28PS ZMM1,[RBP+40h],MASK=K3,ZEROING=ON |00000041:62F27DDBCA4D10<2 | VRCP28PS ZMM1,[RBP+40h],MASK=K3,ZEROING=ON,BCST=ON |00000048:62F2FD5BCACA | VRCP28PD ZMM1,ZMM2,MASK=K3,SAE=ON |0000004E:62F2FDCBCA4D01<6 | VRCP28PD ZMM1,[RBP+40h],MASK=K3,ZEROING=ON |00000055:62F2FDDBCA4D08<3 | VRCP28PD ZMM1,[RBP+40h],MASK=K3,ZEROING=ON,BCST=ON | |ENDPROGRAM t5660`

Expected messages t5660.out
  `I0180 Assembling source file "t5660.htm". I0270 Assembling source "t5660". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5660". "t5660.htm"{58} I0510 Assembling program pass 1. "t5660.htm"{58} I0530 Assembling program pass 2 - final. "t5660.htm"{58} I0660 16bit TINY BIN file "t5660.bin" created, size=92. "t5660.htm"{74} I0650 Program "t5660" assembled in 2 passes with errorlevel 0. "t5660.htm"{74} I0750 Source "t5660" (92 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5660.htm.lst" created, size=1310. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲