| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5292: Machine instructions VEXTRACTI32X4 VEXTRACTI32X8 VEXTRACTI64X2 VEXTRACTI64X4 VEXTRACTI128

Tested procedures
  IizVEXTRACTI32X4 IizVEXTRACTI32X8 IizVEXTRACTI64X2 IizVEXTRACTI64X4 IizVEXTRACTI128

Source & expected listing t5292.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=34, DUMPALL=OFF, CPU=X64, SIMD=AVX512, EVEX=ON | |t5292 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F37D2839D103 | VEXTRACTI32X4 XMM1,YMM2,3 |00000007:62F37D4C39D103 | VEXTRACTI32X4 XMM1,ZMM2,3,MASK=K4 |0000000E:62F37DAC395504<403 | VEXTRACTI32X4 [RBP+40h],YMM2,3,MASK=K4,ZEROING=ON |00000016:62F37D48395504<403 | VEXTRACTI32X4 [RBP+40h],ZMM2,3 |0000001E:62F37D483BD103 | VEXTRACTI32X8 YMM1,ZMM2,3 |00000025:62F37D4C3BD103 | VEXTRACTI32X8 YMM1,ZMM2,3,MASK=K4 |0000002C:62F37DCC3B5502<503 | VEXTRACTI32X8 [RBP+40h],ZMM2,3,MASK=K4,ZEROING=ON |00000034:62F3FD2839D103 | VEXTRACTI64X2 XMM1,YMM2,3 |0000003B:62F3FD4C39D103 | VEXTRACTI64X2 XMM1,ZMM2,3,MASK=K4 |00000042:62F3FDAC395504<403 | VEXTRACTI64X2 [RBP+40h],YMM2,3,MASK=K4,ZEROING=ON |0000004A:62F3FD48395504<403 | VEXTRACTI64X2 [RBP+40h],ZMM2,3 |00000052:62F3FD483BD103 | VEXTRACTI64X4 YMM1,ZMM2,3 |00000059:62F3FD4C3BD103 | VEXTRACTI64X4 YMM1,ZMM2,3,MASK=K4 |00000060:62F3FDCC3B5502<503 | VEXTRACTI64X4 [RBP+40h],ZMM2,3,MASK=K4,ZEROING=ON |00000068:C4E37D39D103 | VEXTRACTI128 XMM1,YMM2,3 |0000006E:C4E37D39554003 | VEXTRACTI128 [RBP+40h],YMM2,3 | |ENDPROGRAM t5292`

Expected messages t5292.out
  `I0180 Assembling source file "t5292.htm". I0270 Assembling source "t5292". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5292". "t5292.htm"{61} I0510 Assembling program pass 1. "t5292.htm"{61} I0530 Assembling program pass 2 - final. "t5292.htm"{61} I0660 16bit TINY BIN file "t5292.bin" created, size=117. "t5292.htm"{79} I0650 Program "t5292" assembled in 2 passes with errorlevel 0. "t5292.htm"{79} I0750 Source "t5292" (97 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5292.htm.lst" created, size=1468. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲