| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3700: Machine instructions LDMXCSR STMXCSR VLDMXCSR VSTMXCSR

Tested procedures
  IipLDMXCSR IipSTMXCSR IiyVLDMXCSR IiyVSTMXCSR

Source & expected listing t3700.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=28,CPU=X64,SIMD=AVX | |t3700 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:0FAE14 | LDMXCSR [SI] |0003:C5F8AE14 | VLDMXCSR [SI] |0007:C4E178AE14 | VLDMXCSR [SI],PREFIX=VEX3 |000C:0FAE1D | STMXCSR [DI] |000F:C5F8AE1D | VSTMXCSR [DI] |0013:C4E178AE1D | VSTMXCSR [DI],PREFIX=VEX3 |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:0FAE16 | LDMXCSR [ESI] |00000003:C5F8AE16 | VLDMXCSR [ESI] |00000007:C4E178AE16 | VLDMXCSR [ESI],PREFIX=VEX3 |0000000C:0FAE1F | STMXCSR [EDI] |0000000F:C5F8AE1F | VSTMXCSR [EDI] |00000013:C4E178AE1F | VSTMXCSR [EDI],PREFIX=VEX3 |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:0FAE16 | LDMXCSR [RSI] |00000003:C5F8AE16 | VLDMXCSR [RSI] |00000007:C4E178AE16 | VLDMXCSR [RSI],PREFIX=VEX3 |0000000C:0FAE1F | STMXCSR [RDI] |0000000F:C5F8AE1F | VSTMXCSR [RDI] |00000013:C4E178AE1F | VSTMXCSR [RDI],PREFIX=VEX3 | |ENDPROGRAM t3700`

Expected messages t3700.out
  `I0180 Assembling source file "t3700.htm". I0270 Assembling source "t3700". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3700". "t3700.htm"{58} I0510 Assembling program pass 1. "t3700.htm"{58} I0530 Assembling program pass 2 - final. "t3700.htm"{58} I0660 16bit TINY BIN file "t3700.bin" created, size=88. "t3700.htm"{80} I0650 Program "t3700" assembled in 2 passes with errorlevel 0. "t3700.htm"{80} I0750 Source "t3700" (98 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3700.htm.lst" created, size=1300. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲