| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3111: Machine instructions OR ORB ORW ORD in 32bit mode

Tested procedures
  IigOR IigORB IigORW IigORD

Source & expected listing t3111.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=36,CPU=386 | |t3111 PROGRAM FORMAT=BIN,IMAGEBASE=0,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:0C02 | OR AL,2 |00000002:80C802 | OR AL,2,CODE=LONG |00000005:660D0200 | OR AX,2 |00000009:6683C802 | OR AX,2,CODE=LONG |0000000D:83C802 | OR EAX,2 |00000010:0D02000000 | OR EAX,2,CODE=SHORT |00000015:80C902 | OR CL,2 |00000018:800D[AE000000]02 | OR [MemByte],2 |0000001F:6683C902 | OR CX,2 |00000023:6681C90200 | OR CX,2,IMM=WORD |00000028:66830D[AC000000]02 | OR [MemWord],2 |00000030:66810D[AC000000]0200 | OR [MemWord],2,IMM=WORD |00000039:810D[AC000000]02000000 | ORD [MemWord],2,IMM=DWORD |00000043:83C902 | OR ECX,2 |00000046:81C902000000 | OR ECX,2,IMM=DWORD |0000004C:830D[A8000000]02 | OR [MemDword],2 |00000053:66830D[A8000000]02 | ORW [MemDword],2 |0000005B:810D[A8000000]02000000 | OR [MemDword],2,IMM=DWORD |00000065:800F02 | ORB [EDI],2 |00000068:66830F02 | ORW [EDI],2 |0000006C:830F02 | ORD [EDI],2 |0000006F:08D1 | OR CL,DL |00000071:0ACA | OR CL,DL,CODE=LONG |00000073:08F5 | OR CH,DH |00000075:0AEE | OR CH,DH,CODE=LONG |00000077:6609D1 | OR CX,DX |0000007A:660BCA | OR CX,DX,CODE=LONG |0000007D:09D1 | OR ECX,EDX |0000007F:0BCA | OR ECX,EDX,CODE=LONG |00000081:0A0D[AE000000] | OR CL,[MemByte] |00000087:660B0D[AC000000] | OR CX,[MemWord] |0000008E:0B0D[A8000000] | OR ECX,[MemDword] |00000094:0815[AE000000] | OR [MemByte],DL |0000009A:660915[AC000000] | OR [MemWord],DX |000000A1:0915[A8000000] | OR [MemDword],EDX |000000A7:90 | ALIGN QWORD |000000A8:00000000 |MemDword D D |000000AC:0000 |MemWord D W |000000AE:00 |MemByte D B | |ENDPROGRAM t3111`

Expected messages t3111.out
  `I0180 Assembling source file "t3111.htm". I0270 Assembling source "t3111". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3111". "t3111.htm"{58} I0510 Assembling program pass 1. "t3111.htm"{58} I0510 Assembling program pass 2. "t3111.htm"{58} I0510 Assembling program pass 3. "t3111.htm"{58} I0530 Assembling program pass 4 - final. "t3111.htm"{58} I0660 16bit TINY BIN file "t3111.bin" created, size=175. "t3111.htm"{99} I0650 Program "t3111" assembled in 4 passes with errorlevel 0. "t3111.htm"{99} I0750 Source "t3111" (119 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3111.htm.lst" created, size=2378. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲