| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3850: Machine instructions MAXSD MAXPD MINSD MINPD MULSD MULPD SQRTSD SQRTPD

Tested procedures
  IipGroupSSE IipMAXSD IipMAXPD IipMINSD IipMINPD IipMULSD IipMULPD IipSQRTSD IipSQRTPD

Source & expected listing t3850.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=32, CPU=X64, SIMD=SSE2 | |t3850 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:F20F5FCF | MAXSD XMM1,XMM7 |0004:F20F5F0C | MAXSD XMM1,[SI] |0008:660F5FCF | MAXPD XMM1,XMM7 |000C:660F5F0C | MAXPD XMM1,[SI] |0010:F20F5DCF | MINSD XMM1,XMM7 |0014:F20F5D0C | MINSD XMM1,[SI] |0018:660F5DCF | MINPD XMM1,XMM7 |001C:660F5D0C | MINPD XMM1,[SI] |0020:F20F59CF | MULSD XMM1,XMM7 |0024:F20F590C | MULSD XMM1,[SI] |0028:660F59CF | MULPD XMM1,XMM7 |002C:660F590C | MULPD XMM1,[SI] |0030:F20F51CF | SQRTSD XMM1,XMM7 |0034:F20F510C | SQRTSD XMM1,[SI] |0038:660F51CF | SQRTPD XMM1,XMM7 |003C:660F510C | SQRTPD XMM1,[SI] |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:F20F5FCF | MAXSD XMM1,XMM7 |00000004:F20F5F0E | MAXSD XMM1,[ESI] |00000008:660F5FCF | MAXPD XMM1,XMM7 |0000000C:660F5F0E | MAXPD XMM1,[ESI] |00000010:F20F5DCF | MINSD XMM1,XMM7 |00000014:F20F5D0E | MINSD XMM1,[ESI] |00000018:660F5DCF | MINPD XMM1,XMM7 |0000001C:660F5D0E | MINPD XMM1,[ESI] |00000020:F20F59CF | MULSD XMM1,XMM7 |00000024:F20F590E | MULSD XMM1,[ESI] |00000028:660F59CF | MULPD XMM1,XMM7 |0000002C:660F590E | MULPD XMM1,[ESI] |00000030:F20F51CF | SQRTSD XMM1,XMM7 |00000034:F20F510E | SQRTSD XMM1,[ESI] |00000038:660F51CF | SQRTPD XMM1,XMM7 |0000003C:660F510E | SQRTPD XMM1,[ESI] |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:F2450F5FCB | MAXSD XMM9,XMM11 |00000005:F2440F5F0E | MAXSD XMM9,[RSI] |0000000A:660F5FCF | MAXPD XMM1,XMM7 |0000000E:66670F5F0E | MAXPD XMM1,[ESI] |00000013:F20F5DCF | MINSD XMM1,XMM7 |00000017:F20F5D0C2500000000 | MINSD XMM1,[0] |00000020:660F5DCF | MINPD XMM1,XMM7 |00000024:6667460F5D5C4DF6 | MINPD XMM11,[2*R9D+EBP-10] |0000002C:F2410F59CB | MULSD XMM1,XMM11 |00000031:F2410F5909 | MULSD XMM1,[R9] |00000036:66410F59CB | MULPD XMM1,XMM11 |0000003B:66410F5909 | MULPD XMM1,[R9] |00000040:F20F51CF | SQRTSD XMM1,XMM7 |00000044:6467F20F510E | SQRTSD XMM1,[FS:ESI] |0000004A:66440F51CF | SQRTPD XMM9,XMM7 |0000004F:66440F510E | SQRTPD XMM9,[RSI] | |ENDPROGRAM t3850`

Expected messages t3850.out
  `I0180 Assembling source file "t3850.htm". I0270 Assembling source "t3850". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3850". "t3850.htm"{73} I0510 Assembling program pass 1. "t3850.htm"{73} I0530 Assembling program pass 2 - final. "t3850.htm"{73} I0660 16bit TINY BIN file "t3850.bin" created, size=212. "t3850.htm"{125} I0650 Program "t3850" assembled in 2 passes with errorlevel 0. "t3850.htm"{125} I0750 Source "t3850" (143 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3850.htm.lst" created, size=2893. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲