| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3066: Machine instructions SAL2 SAL2B SAL2W SAL2D in 32bit mode

Tested procedures
  IigSAL2 IigSAL2B IigSAL2W IigSAL2D

Source & expected listing t3066.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=36,CPU=386 | |t3066 PROGRAM FORMAT=BIN,IMAGEBASE=0,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE | | EUROASM UNDOC=ENABLE |00000000:D2F0 | SAL2 AL,CL |00000002:D0F0 | SAL2 AL |00000004:D0F0 | SAL2 AL,1 |00000006:C0F001 | SAL2 AL,1,CODE=LONG |00000009:C0F001 | SAL2 AL,1,IMM=BYTE |0000000C:C0F002 | SAL2 AL,2 |0000000F:D235[D6000000] | SAL2 [MemByte],CL |00000015:D035[D6000000] | SAL2 [MemByte] |0000001B:D035[D6000000] | SAL2 [MemByte],1 |00000021:C035[D6000000]01 | SAL2 [MemByte],1,CODE=LONG |00000028:C035[D6000000]01 | SAL2 [MemByte],1,IMM=BYTE |0000002F:C035[D6000000]02 | SAL2 [MemByte],2 |00000036:67C03501 | SAL2 [DI],1,DATA=BYTE,IMM=BYTE |0000003A:D037 | SAL2 [EDI],1,DATA=BYTE |0000003C:66D3F0 | SAL2 AX,CL |0000003F:66D1F0 | SAL2 AX |00000042:66D1F0 | SAL2 AX,1 |00000045:66C1F001 | SAL2 AX,1,CODE=LONG |00000049:66C1F001 | SAL2 AX,1,IMM=BYTE |0000004D:66C1F002 | SAL2 AX,2 |00000051:66D335[D4000000] | SAL2 [MemWord],CL |00000058:66D135[D4000000] | SAL2 [MemWord] |0000005F:66D135[D4000000] | SAL2 [MemWord],1 |00000066:66C135[D4000000]01 | SAL2 [MemWord],1,CODE=LONG |0000006E:66C135[D4000000]01 | SAL2 [MemWord],1,IMM=BYTE |00000076:66C135[D4000000]02 | SAL2 [MemWord],2 |0000007E:6667C13501 | SAL2 [DI],1,DATA=WORD,IMM=BYTE |00000083:66D137 | SAL2 [EDI],1,DATA=WORD |00000086:D3F0 | SAL2 EAX,CL |00000088:D1F0 | SAL2 EAX |0000008A:D1F0 | SAL2 EAX,1 |0000008C:C1F001 | SAL2 EAX,1,CODE=LONG |0000008F:C1F001 | SAL2 EAX,1,IMM=BYTE |00000092:C1F002 | SAL2 EAX,2 |00000095:D335[D0000000] | SAL2 [MemDword],CL |0000009B:D135[D0000000] | SAL2 [MemDword] |000000A1:D135[D0000000] | SAL2 [MemDword],1 |000000A7:C135[D0000000]01 | SAL2 [MemDword],1,CODE=LONG |000000AE:C135[D0000000]01 | SAL2 [MemDword],1,IMM=BYTE |000000B5:C135[D0000000]02 | SAL2 [MemDword],2 |000000BC:C13701 | SAL2 [EDI],1,DATA=DWORD,IMM=BYTE |000000BF:67D135 | SAL2 [DI],1,DATA=DWORD |000000C2:D237 | SAL2B [EDI],CL |000000C4:66D337 | SAL2W [EDI],CL |000000C7:D337 | SAL2D [EDI],CL |000000C9:8D842000000000 | ALIGN QWORD |000000D0:00000000 |MemDword D D |000000D4:0000 |MemWord D W |000000D6:00 |MemByte D B | |ENDPROGRAM t3066`

Expected messages t3066.out
  `I0180 Assembling source file "t3066.htm". I0270 Assembling source "t3066". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3066". "t3066.htm"{58} I0510 Assembling program pass 1. "t3066.htm"{58} I0510 Assembling program pass 2. "t3066.htm"{58} I0510 Assembling program pass 3. "t3066.htm"{58} I0530 Assembling program pass 4 - final. "t3066.htm"{58} I0660 16bit TINY BIN file "t3066.bin" created, size=215. "t3066.htm"{110} I0650 Program "t3066" assembled in 4 passes with errorlevel 0. "t3066.htm"{110} I0750 Source "t3066" (130 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3066.htm.lst" created, size=3099. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲