| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3196: Machine instructions POP POPW POPD POPQ with multioperand

Tested procedures
  IiAssembleMultiop IigPOP IigPOPW IigPOPD IigPOPQ

Source & expected listing t3196.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=66,DUMPALL=OFF,CPU=X64 | |t3196 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:58595A5B5C5D5E5F58595A5B | POP AX,CX,DX,BX,SP,BP,SI,DI,AX,CX,DX,BX |000C:8FC08FC18FC28FC38FC48FC58FC68FC7 | POP AX,CX,DX,BX,SP,BP,SI,DI,CODE=LONG |001C:66586659665A665B665C665D665E665F | POP EAX,ECX,EDX,EBX,ESP,EBP,ESI,EDI |002C:668FC0668FC1668FC2668FC3668FC4668FC5 | POP EAX,ECX,EDX,EBX,ESP,EBP,CODE=LONG |003E:5807665B8F06[9400]8F05 | POP AX,ES,EBX,[MemWord],[DI] |0048:8F058F06[9400]668F06[9000]8F06[4800] | POP [DI],[MemWord],[MemDword],[$] |0057:668F05668F06[9400]668F06[9000]668F06[5700] | POP [DI],[MemWord],[MemDword],[$],DATA=DWORD |0069:8F058F06[9400]8F06[9000]8F06[8800] | POPW [DI],[MemWord],[MemDword],[MemQword] |0077:668F05668F06[9400]668F06[9000]668F06[8800] | POPD [DI],[MemWord],[MemDword],[MemQword] |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:66586659665A665B665C665D665E665F | POP AX,CX,DX,BX,SP,BP,SI,DI |00000010:668FC0668FC1668FC2668FC3668FC4668FC5 | POP AX,CX,DX,BX,SP,BP,CODE=LONG |00000022:58595A5B5C5D5E5F58595A5B | POP EAX,ECX,EDX,EBX,ESP,EBP,ESI,EDI,EAX,ECX,EDX,EBX |0000002E:8FC08FC18FC28FC38FC48FC58FC68FC7 | POP EAX,ECX,EDX,EBX,ESP,EBP,ESI,EDI,CODE=LONG |0000003E:6658075B8F05[90000000]678F05 | POP AX,ES,EBX,[MemDword],[DI] |0000004B:668F05[94000000]8F05[90000000]8F05[4B000000] | POP [MemWord],[MemDword],[$] |0000005E:668F07668F05[94000000]668F05[90000000]668F05[88000000] | POPW [EDI],[MemWord],[MemDword],[MemQword] |00000076:8F078F05[94000000]8F05[90000000]8F05[88000000] | POPD [EDI],[MemWord],[MemDword],[MemQword] |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:58595A5B5C5D5E5F4159415A | POP RAX,RCX,RDX,RBX,RSP,RBP,RSI,RDI,R9,R10 |0000000C:8FC08FC18FC28FC38FC48FC58FC68FC7 | POP RAX,RCX,RDX,RBX,RSP,RBP,RSI,RDI,CODE=LONG |0000001C:6658665966415B66415C | POP AX,CX,R11W,R12W |00000026:668FC0668FC166418FC366418FC4 | POP AX,CX,R11W,R12W,CODE=LONG |00000034:66580FA158668F05540000008F0542000000 | POP AX,FS,RAX,[MemWord],[MemQword] |00000046:8F07668F05450000008F05330000008F05EBFFFFFF | POP [RDI],[MemWord],[MemQword],[$] |0000005B:668F07668F052F000000668F0524000000668F0515000000 | POPW [RDI],[MemWord],[MemDword],[MemQword] |00000073:8F078F05190000008F050F0000008F0501000000 | POPQ [RDI],[MemWord],[MemDword],[MemQword] |00000087:90 | ALIGN QWORD |00000088:0000000000000000 |MemQword D Q |00000090:00000000 |MemDword D D |00000094:0000 |MemWord D W | | ENDPROGRAM t3196`

Expected messages t3196.out
  `I0180 Assembling source file "t3196.htm". I0270 Assembling source "t3196". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3196". "t3196.htm"{61} I0510 Assembling program pass 1. "t3196.htm"{61} I0510 Assembling program pass 2. "t3196.htm"{61} I0530 Assembling program pass 3 - final. "t3196.htm"{61} I0660 16bit TINY BIN file "t3196.bin" created, size=438. "t3196.htm"{94} I0650 Program "t3196" assembled in 3 passes with errorlevel 0. "t3196.htm"{94} I0750 Source "t3196" (113 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3196.htm.lst" created, size=3617. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲