| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3052: Machine instructions RCL RCLB RCLW RCLD in 16bit mode

Tested procedures
  IigRCL IigRCLB IigRCLW IigRCLD

Source & expected listing t3052.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=36,CPU=386 | |t3052 PROGRAM FORMAT=BIN,IMAGEBASE=0,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:D2D0 | RCL AL,CL |0002:D0D0 | RCL AL |0004:D0D0 | RCL AL,1 |0006:C0D001 | RCL AL,1,CODE=LONG |0009:C0D001 | RCL AL,1,IMM=BYTE |000C:C0D002 | RCL AL,2 |000F:D216[AE00] | RCL [MemByte],CL |0013:D016[AE00] | RCL [MemByte] |0017:D016[AE00] | RCL [MemByte],1 |001B:C016[AE00]01 | RCL [MemByte],1,CODE=LONG |0020:C016[AE00]01 | RCL [MemByte],1,IMM=BYTE |0025:C016[AE00]02 | RCL [MemByte],2 |002A:C01501 | RCL [DI],1,DATA=BYTE,IMM=BYTE |002D:67D017 | RCL [EDI],1,DATA=BYTE |0030:D3D0 | RCL AX,CL |0032:D1D0 | RCL AX |0034:D1D0 | RCL AX,1 |0036:C1D001 | RCL AX,1,CODE=LONG |0039:C1D001 | RCL AX,1,IMM=BYTE |003C:C1D002 | RCL AX,2 |003F:D316[AC00] | RCL [MemWord],CL |0043:D116[AC00] | RCL [MemWord] |0047:D116[AC00] | RCL [MemWord],1 |004B:C116[AC00]01 | RCL [MemWord],1,CODE=LONG |0050:C116[AC00]01 | RCL [MemWord],1,IMM=BYTE |0055:C116[AC00]02 | RCL [MemWord],2 |005A:C11501 | RCL [DI],1,DATA=WORD,IMM=BYTE |005D:67D117 | RCL [EDI],1,DATA=WORD |0060:66D3D0 | RCL EAX,CL |0063:66D1D0 | RCL EAX |0066:66D1D0 | RCL EAX,1 |0069:66C1D001 | RCL EAX,1,CODE=LONG |006D:66C1D001 | RCL EAX,1,IMM=BYTE |0071:66C1D002 | RCL EAX,2 |0075:66D316[A800] | RCL [MemDword],CL |007A:66D116[A800] | RCL [MemDword] |007F:66D116[A800] | RCL [MemDword],1 |0084:66C116[A800]01 | RCL [MemDword],1,CODE=LONG |008A:66C116[A800]01 | RCL [MemDword],1,IMM=BYTE |0090:66C116[A800]02 | RCL [MemDword],2 |0096:66C11501 | RCL [DI],1,DATA=DWORD,IMM=BYTE |009A:6667D117 | RCL [EDI],1,DATA=DWORD |009E:D215 | RCLB [DI],CL |00A0:D315 | RCLW [DI],CL |00A2:66D315 | RCLD [DI],CL |00A5:9087C9 | ALIGN QWORD |00A8:00000000 |MemDword D D |00AC:0000 |MemWord D W |00AE:00 |MemByte D B | |ENDPROGRAM t3052`

Expected messages t3052.out
  `I0180 Assembling source file "t3052.htm". I0270 Assembling source "t3052". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3052". "t3052.htm"{58} I0510 Assembling program pass 1. "t3052.htm"{58} I0510 Assembling program pass 2. "t3052.htm"{58} I0510 Assembling program pass 3. "t3052.htm"{58} I0530 Assembling program pass 4 - final. "t3052.htm"{58} I0660 16bit TINY BIN file "t3052.bin" created, size=175. "t3052.htm"{109} I0650 Program "t3052" assembled in 4 passes with errorlevel 0. "t3052.htm"{109} I0750 Source "t3052" (129 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3052.htm.lst" created, size=2992. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲