| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3262: Machine instructions TEST TESTB TESTW TESTD TEST2 TEST2B TEST2W TEST2D in 32bit mode

Tested procedures
  IigTEST IigTESTB IigTESTW IigTESTD IigTEST2 IigTEST2B IigTEST2W IigTEST2D

Source & expected listing t3262.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=38, CPU=386 | |t3262 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:A802 | TEST AL,2 |00000002:F6C002 | TEST AL,2,CODE=LONG |00000005:F6C102 | TEST CL,2 |00000008:66A90200 | TEST AX,2 |0000000C:66F7C00200 | TEST AX,2,CODE=LONG |00000011:66F7C10200 | TEST CX,2 |00000016:A902000000 | TEST EAX,2 |0000001B:F7C002000000 | TEST EAX,2,CODE=LONG |00000021:F7C102000000 | TEST ECX,2 |00000027:84C9 | TEST CL |00000029:84C9 | TEST CL,CL |0000002B:84D1 | TEST CL,DL |0000002D:84CA | TEST CL,DL,CODE=LONG |0000002F:6685C9 | TEST CX |00000032:6685D1 | TEST CX,DX |00000035:6685CA | TEST CX,DX,CODE=LONG |00000038:85C9 | TEST ECX |0000003A:85D1 | TEST ECX,EDX |0000003C:85CA | TEST ECX,EDX,CODE=LONG |0000003E:F605[EE000000]02 | TEST [MemByte],2 |00000045:66F705[EC000000]0200 | TEST [MemWord],2 |0000004E:F705[E8000000]02000000 | TEST [MemDword],2 |00000058:F60602 | TESTB [ESI],2 |0000005B:66F7060200 | TESTW [ESI],2 |00000060:F70602000000 | TESTD [ESI],2 |00000066:8416 | TEST [ESI],DL |00000068:8416 | TEST DL,[ESI] |0000006A:668516 | TEST [ESI],DX |0000006D:668516 | TEST DX,[ESI] |00000070:8516 | TEST [ESI],EDX |00000072:8516 | TEST EDX,[ESI] | | EUROASM UNDOC=ENABLE |00000074:A802 | TEST2 AL,2 |00000076:F6C802 | TEST2 AL,2,CODE=LONG |00000079:F6C902 | TEST2 CL,2 |0000007C:66A90200 | TEST2 AX,2 |00000080:66F7C80200 | TEST2 AX,2,CODE=LONG |00000085:66F7C90200 | TEST2 CX,2 |0000008A:A902000000 | TEST2 EAX,2 |0000008F:F7C802000000 | TEST2 EAX,2,CODE=LONG |00000095:F7C902000000 | TEST2 ECX,2 |0000009B:84C9 | TEST2 CL |0000009D:84C9 | TEST2 CL,CL |0000009F:84D1 | TEST2 CL,DL |000000A1:84CA | TEST2 CL,DL,CODE=LONG |000000A3:6685C9 | TEST2 CX |000000A6:6685D1 | TEST2 CX,DX |000000A9:6685CA | TEST2 CX,DX,CODE=LONG |000000AC:85C9 | TEST2 ECX |000000AE:85D1 | TEST2 ECX,EDX |000000B0:85CA | TEST2 ECX,EDX,CODE=LONG |000000B2:F60D[EE000000]02 | TEST2 [MemByte],2 |000000B9:66F70D[EC000000]0200 | TEST2 [MemWord],2 |000000C2:F70D[E8000000]02000000 | TEST2 [MemDword],2 |000000CC:F60E02 | TEST2B [ESI],2 |000000CF:66F70E0200 | TEST2W [ESI],2 |000000D4:F70E02000000 | TEST2D [ESI],2 |000000DA:8416 | TEST2 [ESI],DL |000000DC:8416 | TEST2 DL,[ESI] |000000DE:668516 | TEST2 [ESI],DX |000000E1:668516 | TEST2 DX,[ESI] |000000E4:8516 | TEST2 [ESI],EDX |000000E6:8516 | TEST2 EDX,[ESI] |000000E8: | ALIGN QWORD |000000E8:00000000 |MemDword D D |000000EC:0000 |MemWord D W |000000EE:00 |MemByte D B | | ENDPROGRAM t3262`

Expected messages t3262.out
  `I0180 Assembling source file "t3262.htm". I0270 Assembling source "t3262". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3262". "t3262.htm"{70} I0510 Assembling program pass 1. "t3262.htm"{70} I0510 Assembling program pass 2. "t3262.htm"{70} I0510 Assembling program pass 3. "t3262.htm"{70} I0530 Assembling program pass 4 - final. "t3262.htm"{70} I0660 16bit TINY BIN file "t3262.bin" created, size=239. "t3262.htm"{139} I0650 Program "t3262" assembled in 4 passes with errorlevel 0. "t3262.htm"{139} I0750 Source "t3262" (159 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3262.htm.lst" created, size=3975. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲