| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3212: Machine instructions SCAS SCASB SCASW SCASD SCASQ

Tested procedures
  IigSCAS IigSCASB IigSCASW IigSCASD IigSCASQ

Source & expected listing t3212.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=30, CPU=X64 | |t3212 PROGRAM FORMAT=BIN,LISTMAP=OFF,LISTGLOBALS=OFF | |;; |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:AE | SCASB |0001:AF | SCASW |0002:66AF | SCASD |0004:F3AF | REP SCASW |0006:F3AF | REPE SCASW |0008:F2AF | REPNE SCASW |000A:AE | SCAS AL,[DI] |000B:AF | SCAS AX,[DI] |000C:66AF | SCAS EAX,[DI] |000E:AE | SCAS DATA=BYTE |000F:AF | SCAS DATA=WORD |0010:66AF | SCAS DATA=DWORD |0012:AF | SCASW [DI] |0013:67AF | SCASW [EDI] |0015:AF | SCASW [ES:DI] |0016:67AF | SCASW [ES:EDI] |0018:26AF | SEGES SCASW |001A:AE | SCAS [MemByte] |001B:AF | SCAS [MemWord] |001C:66AF | SCAS [MemDword] |001E:AF | SCAS AX,[MemQword] |001F:AE | SCAS [DI+MemByte] |0020:AF | SCAS [DI+MemWord] |0021:66AF | SCAS [DI+MemDword] | |;; |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:AE | SCASB |00000001:66AF | SCASW |00000003:AF | SCASD |00000004:F366AF | REP SCASW |00000007:F366AF | REPE SCASW |0000000A:F266AF | REPNE SCASW |0000000D:AE | SCAS AL,[EDI] |0000000E:66AF | SCAS AX,[EDI] |00000010:AF | SCAS EAX,[EDI] |00000011:AE | SCAS DATA=BYTE |00000012:66AF | SCAS DATA=WORD |00000014:AF | SCAS DATA=DWORD |00000015:66AF | SCASW [EDI] |00000017:6667AF | SCASW [DI] |0000001A:6667AF | SCASW [ES:DI] |0000001D:66AF | SCASW [ES:EDI] |0000001F:2666AF | SEGES SCASW |00000022:AE | SCAS [MemByte] |00000023:66AF | SCAS [MemWord] |00000025:AF | SCAS [MemDword] |00000026:AF | SCAS EAX,[MemQword] |00000027:AE | SCAS [EDI+MemByte] |00000028:66AF | SCAS [EDI+MemWord] |0000002A:AF | SCAS [EDI+MemDword] | |;; |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:AE | SCASB |00000001:66AF | SCASW |00000003:AF | SCASD |00000004:48AF | SCASQ |00000006:F348AF | REP SCASQ |00000009:F348AF | REPE SCASQ |0000000C:F248AF | REPNE SCASQ |0000000F:AE | SCAS AL,[RDI] |00000010:66AF | SCAS AX,[RDI] |00000012:AF | SCAS EAX,[RDI] |00000013:48AF | SCAS RAX,[RDI] |00000015:AE | SCAS DATA=BYTE |00000016:66AF | SCAS DATA=WORD |00000018:AF | SCAS DATA=DWORD |00000019:48AF | SCAS DATA=QWORD |0000001B:66AF | SCASW [RDI] |0000001D:6667AF | SCASW [EDI] |00000020:AE | SCAS [MemByte] |00000021:66AF | SCAS [MemWord] |00000023:AF | SCAS [MemDword] |00000024:48AF | SCAS [MemQword] |00000026:AE | SCAS [RDI+MemByte] |00000027:66AF | SCAS [RDI+MemWord] |00000029:AF | SCAS [RDI+MemDword] |0000002A:48AF | SCAS [RDI+MemQword] |0000002C:0F1F4000 | ALIGN QWORD |00000030:0000000000000000 |MemQword DQ Q |00000038:00000000 |MemDword DD D |0000003C:0000 |MemWord DW W |0000003E:00 |MemByte DB B | | ENDPROGRAM t3212`

Expected messages t3212.out
  `I0180 Assembling source file "t3212.htm". I0270 Assembling source "t3212". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3212". "t3212.htm"{61} I0510 Assembling program pass 1. "t3212.htm"{61} I0510 Assembling program pass 2. "t3212.htm"{61} I0510 Assembling program pass 3. "t3212.htm"{61} I0530 Assembling program pass 4 - final. "t3212.htm"{61} I0660 16bit TINY BIN file "t3212.bin" created, size=159. "t3212.htm"{146} I0650 Program "t3212" assembled in 4 passes with errorlevel 0. "t3212.htm"{146} I0750 Source "t3212" (166 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3212.htm.lst" created, size=4075. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲