| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t4675: Machine instructions VFNMADDSS VFNMADDSD VFNMSUBSS VFNMSUBSD

Tested procedures
  IiaVFNMADDSS IiaVFNMADDSD IiaVFNMSUBSS IiaVFNMSUBSD

Source & expected listing t4675.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=24,CPU=X64,SIMD=AVX,FMA=ON,AMD=ON | |t4675 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C4E3697A0E40 | VFNMADDSS XMM1,XMM2,[RSI],XMM4 |00000006:C4E3697B0E40 | VFNMADDSD XMM1,XMM2,[RSI],XMM4 |0000000C:C4E3697E0E40 | VFNMSUBSS XMM1,XMM2,[RSI],XMM4 |00000012:C4E3697F0E40 | VFNMSUBSD XMM1,XMM2,[RSI],XMM4 |00000018:C4E3E97A0E30 | VFNMADDSS XMM1,XMM2,XMM3,[RSI] |0000001E:C4E3E97B0E30 | VFNMADDSD XMM1,XMM2,XMM3,[RSI] |00000024:C4E3E97E0E30 | VFNMSUBSS XMM1,XMM2,XMM3,[RSI] |0000002A:C4E3E97F0E30 | VFNMSUBSD XMM1,XMM2,XMM3,[RSI] |00000030:C4E3697ACB40 | VFNMADDSS XMM1,XMM2,XMM3,XMM4 |00000036:C4E3697BCB40 | VFNMADDSD XMM1,XMM2,XMM3,XMM4 |0000003C:C4E3697ECB40 | VFNMSUBSS XMM1,XMM2,XMM3,XMM4 |00000042:C4E3697FCB40 | VFNMSUBSD XMM1,XMM2,XMM3,XMM4 |00000048:C4E3E97ACC30 | VFNMADDSS XMM1,XMM2,XMM3,XMM4,CODE=LONG |0000004E:C4E3E97BCC30 | VFNMADDSD XMM1,XMM2,XMM3,XMM4,CODE=LONG |00000054:C4E3E97ECC30 | VFNMSUBSS XMM1,XMM2,XMM3,XMM4,CODE=LONG |0000005A:C4E3E97FCC30 | VFNMSUBSD XMM1,XMM2,XMM3,XMM4,CODE=LONG | |ENDPROGRAM t4675`

Expected messages t4675.out
  `I0180 Assembling source file "t4675.htm". I0270 Assembling source "t4675". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t4675". "t4675.htm"{58} I0510 Assembling program pass 1. "t4675.htm"{58} I0530 Assembling program pass 2 - final. "t4675.htm"{58} I0660 16bit TINY BIN file "t4675.bin" created, size=96. "t4675.htm"{76} I0650 Program "t4675" assembled in 2 passes with errorlevel 0. "t4675.htm"{76} I0750 Source "t4675" (94 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t4675.htm.lst" created, size=1225. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲