| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t8000: BIN program for 16bit BIOS

Tested procedures
  PfbinCompile

Source & expected listing t8000.htm.lst
  `| | EUROASM AUTOSEGMENT=ON,CPU=086,DUMPWIDTH=24,PRIV=ENABLED |7438303030 |%test %SET t8000 ; BIN.B16 | |;; | |%test PROGRAM FORMAT=BIN,WIDTH=16,MODEL=TINY |[CODE] ::::Section changed. |0000:90 | NOP |0001:BE[0000] | MOV SI,Msg |0004:E80600 | CALL Write.B16:: |0007:E81200 | CALL Beep.B16:: |000A:E81C00 | CALL Exit.B16:: |[DATA] ::::Section changed. |0000:3136626974205449~|Msg:DB '%^WIDTH[]bit %^MODEL %^FORMAT program "%^OUTFILE".',13,10,0 | |;; |[CODE] ::::Section changed. |000D: |Write.B16:: PROC ; Display ASCIIZ string pointed to by DS:SI using BIOS. |000D:31DB | XOR BX,BX ; Videopage=0. |000F:B40E | MOV AH,0Eh ; BIOS service Teletype output. |0011:FC | CLD ; Direction forward. |0012:AC |.1:LODSB ; Load a character from string to AL, increment SI. |0013:3C00 | CMP AL,0 ; Test if zero-terminator reached. |0015:7404 | JE .9: ; Exit the procedure if AL=0. |0017:CD10 | INT 10h ; Otherwise display the character AL and advance screen cursor. |0019:EBF7 | JMP .1: ; Repeat with following characters. |001B:C3 |.9:RET ; AX,BX,SI are clobbered. |001C: | ENDP Write.B16:: | |;; |001C: |Beep.B16:: PROC ; Display message "Beeping.." and play a sound using BIOS. |001C:BE[0000] | MOV SI,=B"Beeping..." ; Define a literal string. Assume DS=PARA# [RODATA}. |001F:E8EBFF | CALL Write.B16:: ; Display the notification "Beeping...". |0022:BE[0000] | MOV SI,=W(0x0007) ; Define ASCIIZ string with BEL character in [RODATA]. |0025:E8E5FF | CALL Write.B16:: ; Play the beep sound. |0028:C3 | RET ; AX,BX,SI are clobbered. |0029: | ENDP Beep.B16:: | |;; |0029: |Exit.B16:: PROC ; Display message "End", terminate Terminate the program by endless loop. |0029:BE[0000] | MOV SI,.M: ; String "End" will be defined in segment [BSS] at DS:SI. |002C:C704456E | MOVW [SI+0],"En" ; Dynamically initialize the notification string. |0030:C744026420 | MOVW [SI+2],"d " ; Assume DS=PARA# [BSS]. |0035:C744040A0D | MOVW [SI+4],0x0D0A ; CR+LF. |003A:C6440600 | MOVB [SI+6],0 ; Zero-terminate the notification. |003E:E8CCFF | CALL Write.B16:: ; Display notification "End". |0041:F4 |.9:HLT ; Assume there is no OS to return. |0042:EBFD | JMP .9: ; Terminate in endless loop. |[BSS] ::::Section changed. |0000:.............. |.M:DB 7*BYTE ; Reserve space for ASCIIZ string "End" in [BSS] segment. |[CODE] ::::Section changed. |0044: | ENDP Exit.B16:: |[@LT2] ====ListLiterals in section [@LT2]. |0000:0700 =W(0x0007) |[@LT1] ====ListLiterals in section [@LT1]. |0000:42656570696E672E~=B"Beeping..." | | ENDPROGRAM %test | **** ListMap "t8000.bin",model=TINY,groups=1,segments=4,entry=,stack=[COMGROUP]:0000FFFEh | [COMGROUP],FA=00000000h,VA=00000000h,size=00000097h=151,group [CODE] [RODATA] [DATA] [BSS] | [CODE],FA=00000000h,VA=00000000h,size=00000044h=68,width=16,align=0010h,purpose=CODE | [RODATA],FA=00000050h,VA=00000050h,size=0000000Dh=13,width=16,align=0010h,purpose=RODATA+LITERAL | [DATA],FA=00000060h,VA=00000060h,size=00000026h=38,width=16,align=0010h,purpose=DATA | [BSS],FA=00000090h,VA=00000090h,size=00000007h=7,width=16,align=0010h,purpose=BSS | **** ListGlobals "t8000.bin",Global=0,Public=3,Extern=0,eXport=0,Import=0 | Beep.B16,[COMGROUP]:0000001Ch,VA=0000001Ch,scope='P' | Exit.B16,[COMGROUP]:00000029h,VA=00000029h,scope='P' | Write.B16,[COMGROUP]:0000000Dh,VA=0000000Dh,scope='P'`

Expected messages t8000.out
  `I0180 Assembling source file "t8000.htm". I0270 Assembling source "t8000". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t8000". "t8000.htm"{51} I0510 Assembling program pass 1. "t8000.htm"{51} I0510 Assembling program pass 2. "t8000.htm"{51} I0530 Assembling program pass 3 - final. "t8000.htm"{51} I0660 16bit TINY BIN file "t8000.bin" created, size=134. "t8000.htm"{99} I0650 Program "t8000" assembled in 3 passes with errorlevel 0. "t8000.htm"{99} I0750 Source "t8000" (141 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t8000.htm.lst" created, size=4423. I0990 EuroAssembler terminated with errorlevel 0.`

Expected output file t8000. bin

      0000: 90 BE 60 00 E8 06 00 E8 12 00 E8 1C 00 31 DB B4  ¤¤`°¤·°¤·°¤·°1¤¤
      0010: 0E FC AC 3C 00 74 04 CD 10 EB F7 C3 BE 52 00 E8  ·¤¤<°t·¤·¤¤¤¤R°¤
      0020: EB FF BE 50 00 E8 E5 FF C3 BE 90 00 C7 04 45 6E  ¤¤¤P°¤¤¤¤¤¤°¤·En
      0030: C7 44 02 64 20 C7 44 04 0A 0D C6 44 06 00 E8 CC  ¤D·d¯¤D·¬·¤D·°¤¤
      0040: FF F4 EB FD 00 00 00 00 00 00 00 00 00 00 00 00  ¤¤¤¤°°°°°°°°°°°°
      0050: 07 00 42 65 65 70 69 6E 67 2E 2E 2E 00 00 00 00  ·°Beeping...°°°°
      0060: 31 36 62 69 74 20 54 49 4E 59 20 42 49 4E 20 70  16bit¯TINY¯BIN¯p
      0070: 72 6F 67 72 61 6D 20 22 74 38 30 30 30 2E 62 69  rogram¯"t8000.bi
      0080: 6E 22 2E 0D 0A 00                                n".·¬°

▲Back to the top▲