| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3062: Machine instructions RCL RCLB RCLW RCLD in 32bit mode

Tested procedures
  IigRCL IigRCLB IigRCLW IigRCLD

Source & expected listing t3062.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=36,CPU=386 | |t3062 PROGRAM FORMAT=BIN,IMAGEBASE=0,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:D2D0 | RCL AL,CL |00000002:D0D0 | RCL AL |00000004:D0D0 | RCL AL,1 |00000006:C0D001 | RCL AL,1,CODE=LONG |00000009:C0D001 | RCL AL,1,IMM=BYTE |0000000C:C0D002 | RCL AL,2 |0000000F:D215[D6000000] | RCL [MemByte],CL |00000015:D015[D6000000] | RCL [MemByte] |0000001B:D015[D6000000] | RCL [MemByte],1 |00000021:C015[D6000000]01 | RCL [MemByte],1,CODE=LONG |00000028:C015[D6000000]01 | RCL [MemByte],1,IMM=BYTE |0000002F:C015[D6000000]02 | RCL [MemByte],2 |00000036:67C01501 | RCL [DI],1,DATA=BYTE,IMM=BYTE |0000003A:D017 | RCL [EDI],1,DATA=BYTE |0000003C:66D3D0 | RCL AX,CL |0000003F:66D1D0 | RCL AX |00000042:66D1D0 | RCL AX,1 |00000045:66C1D001 | RCL AX,1,CODE=LONG |00000049:66C1D001 | RCL AX,1,IMM=BYTE |0000004D:66C1D002 | RCL AX,2 |00000051:66D315[D4000000] | RCL [MemWord],CL |00000058:66D115[D4000000] | RCL [MemWord] |0000005F:66D115[D4000000] | RCL [MemWord],1 |00000066:66C115[D4000000]01 | RCL [MemWord],1,CODE=LONG |0000006E:66C115[D4000000]01 | RCL [MemWord],1,IMM=BYTE |00000076:66C115[D4000000]02 | RCL [MemWord],2 |0000007E:6667C11501 | RCL [DI],1,DATA=WORD,IMM=BYTE |00000083:66D117 | RCL [EDI],1,DATA=WORD |00000086:D3D0 | RCL EAX,CL |00000088:D1D0 | RCL EAX |0000008A:D1D0 | RCL EAX,1 |0000008C:C1D001 | RCL EAX,1,CODE=LONG |0000008F:C1D001 | RCL EAX,1,IMM=BYTE |00000092:C1D002 | RCL EAX,2 |00000095:D315[D0000000] | RCL [MemDword],CL |0000009B:D115[D0000000] | RCL [MemDword] |000000A1:D115[D0000000] | RCL [MemDword],1 |000000A7:C115[D0000000]01 | RCL [MemDword],1,CODE=LONG |000000AE:C115[D0000000]01 | RCL [MemDword],1,IMM=BYTE |000000B5:C115[D0000000]02 | RCL [MemDword],2 |000000BC:C11701 | RCL [EDI],1,DATA=DWORD,IMM=BYTE |000000BF:67D115 | RCL [DI],1,DATA=DWORD |000000C2:D217 | RCLB [EDI],CL |000000C4:66D317 | RCLW [EDI],CL |000000C7:D317 | RCLD [EDI],CL |000000C9:8D842000000000 | ALIGN QWORD |000000D0:00000000 |MemDword D D |000000D4:0000 |MemWord D W |000000D6:00 |MemByte D B | |ENDPROGRAM t3062`

Expected messages t3062.out
  `I0180 Assembling source file "t3062.htm". I0270 Assembling source "t3062". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3062". "t3062.htm"{58} I0510 Assembling program pass 1. "t3062.htm"{58} I0510 Assembling program pass 2. "t3062.htm"{58} I0510 Assembling program pass 3. "t3062.htm"{58} I0530 Assembling program pass 4 - final. "t3062.htm"{58} I0660 16bit TINY BIN file "t3062.bin" created, size=215. "t3062.htm"{109} I0650 Program "t3062" assembled in 4 passes with errorlevel 0. "t3062.htm"{109} I0750 Source "t3062" (129 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3062.htm.lst" created, size=2995. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲