| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t4565: Machine instructions VPCOMQ VPCOMLTQ VPCOMLEQ VPCOMGTQ VPCOMGEQ VPCOMEQQ VPCOMNEQQ VPCOMFALSEQ VPCOMTRUEQ

Tested procedures
  IixVPCOMQ IixVPCOMLTQ IixVPCOMLEQ IixVPCOMGTQ IixVPCOMGEQ IixVPCOMEQQ IixVPCOMNEQQ IixVPCOMFALSEQ IixVPCOMTRUEQ

Source & expected listing t4565.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=24,CPU=X64,SIMD=AVX,AMD=ON,XOP=ON,PROT=ON | |t4565 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:8FE868CFCB04 | VPCOMQ XMM1,XMM2,XMM3,4 |00000006:8FE868CFCB00 | VPCOMLTQ XMM1,XMM2,XMM3 |0000000C:8FE868CFCB01 | VPCOMLEQ XMM1,XMM2,XMM3 |00000012:8FE868CFCB02 | VPCOMGTQ XMM1,XMM2,XMM3 |00000018:8FE868CFCB03 | VPCOMGEQ XMM1,XMM2,XMM3 |0000001E:8FE868CFCB04 | VPCOMEQQ XMM1,XMM2,XMM3 |00000024:8FE868CFCB05 | VPCOMNEQQ XMM1,XMM2,XMM3 |0000002A:8FE868CFCB06 | VPCOMFALSEQ XMM1,XMM2,XMM3 |00000030:8FE868CFCB07 | VPCOMTRUEQ XMM1,XMM2,XMM3 |00000036:8FE868CF0E04 | VPCOMQ XMM1,XMM2,[RSI],4 |0000003C:8FE868CF0E00 | VPCOMLTQ XMM1,XMM2,[RSI] |00000042:8FE868CF0E01 | VPCOMLEQ XMM1,XMM2,[RSI] |00000048:8FE868CF0E02 | VPCOMGTQ XMM1,XMM2,[RSI] |0000004E:8FE868CF0E03 | VPCOMGEQ XMM1,XMM2,[RSI] |00000054:8FE868CF0E04 | VPCOMEQQ XMM1,XMM2,[RSI] |0000005A:8FE868CF0E05 | VPCOMNEQQ XMM1,XMM2,[RSI] |00000060:8FE868CF0E06 | VPCOMFALSEQ XMM1,XMM2,[RSI] |00000066:8FE868CF0E07 | VPCOMTRUEQ XMM1,XMM2,[RSI] | |ENDPROGRAM t4565`

Expected messages t4565.out
  `I0180 Assembling source file "t4565.htm". I0270 Assembling source "t4565". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t4565". "t4565.htm"{73} I0510 Assembling program pass 1. "t4565.htm"{73} I0530 Assembling program pass 2 - final. "t4565.htm"{73} I0660 16bit TINY BIN file "t4565.bin" created, size=108. "t4565.htm"{93} I0650 Program "t4565" assembled in 2 passes with errorlevel 0. "t4565.htm"{93} I0750 Source "t4565" (111 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t4565.htm.lst" created, size=1257. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲