| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5242: Machine instructions VBROADCASTF32X2 VBROADCASTF32X4 VBROADCASTF32X8 VBROADCASTF64X2 VBROADCASTF64X4

Tested procedures
  IizVBROADCASTF32X2 IizVBROADCASTF32X4 IizVBROADCASTF32X8 IizVBROADCASTF64X2 IizVBROADCASTF64X4

Source & expected listing t5242.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=30, CPU=X64, SIMD=AVX512, MVEX=ON, EVEX=ON | |t5242 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F27D2819CA | VBROADCASTF32X2 YMM1,XMM2 |00000006:62F27DCB19CA | VBROADCASTF32X2 ZMM1,XMM2,MASK=K3,ZEROING=ON |0000000C:62F27D28194D08<3 | VBROADCASTF32X2 YMM1,[RBP+40h] |00000013:62F27D48194D08<3 | VBROADCASTF32X2 ZMM1,[RBP+40h] |0000001A:62F27D4A1A4D04<4 | VBROADCASTF32X4 ZMM1,[RBP+40h],MASK=K2 |00000021:62F2798A1A4D04<4 | VBROADCASTF32X4 ZMM1,[RBP+40h],MASK=K2,EH=ON |00000028:62F27D4A1B4D02<5 | VBROADCASTF32X8 ZMM1,[RBP+40h],MASK=K2 |0000002F:62F2FD2A1A4D04<4 | VBROADCASTF64X2 YMM1,[RBP+40h],MASK=K2 |00000036:62F2FDCA1A4D04<4 | VBROADCASTF64X2 ZMM1,[RBP+40h],MASK=K2,ZEROING=ON |0000003D:62F2FD4A1B4D02<5 | VBROADCASTF64X4 ZMM1,[RBP+40h],MASK=K2 |00000044:62F2F98A1B4D02<5 | VBROADCASTF64X4 ZMM1,[RBP+40h],MASK=K2,EH=ON | |ENDPROGRAM t5242`

Expected messages t5242.out
  `I0180 Assembling source file "t5242.htm". I0270 Assembling source "t5242". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5242". "t5242.htm"{61} I0510 Assembling program pass 1. "t5242.htm"{61} I0530 Assembling program pass 2 - final. "t5242.htm"{61} I0660 16bit TINY BIN file "t5242.bin" created, size=75. "t5242.htm"{74} I0650 Program "t5242" assembled in 2 passes with errorlevel 0. "t5242.htm"{74} I0750 Source "t5242" (92 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5242.htm.lst" created, size=1096. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲