| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5446: Machine instructions VGATHERPF1DPS VGATHERPF1QPS VGATHERPF1DPD VGATHERPF1QPD

Tested procedures
  IizVGATHERPF1DPS IizVGATHERPF1QPS IizVGATHERPF1DPD IizVGATHERPF1QPD

Source & expected listing t5446.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,DUMPALL=OFF,CPU=X64,SIMD=AVX512,EVEX=ON,MVEX=ON | |t5446 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F27D4AC7540D10<2 | VGATHERPF1QPS [ZMM1+RBP+40h],MASK=K2 |00000008:62F2FD4AC7540D08<3 | VGATHERPF1QPD [ZMM1+RBP+40h],MASK=K2 |00000010:62F2FD4AC6540D08<3 | VGATHERPF1DPD [YMM1+RBP+40h],MASK=K2 |00000018:62F27D4AC6540D10<2 | VGATHERPF1DPS [ZMM1+RBP+40h],MASK=K2 |00000020:62F2790AC6540D10<2 | VGATHERPF1DPS [ZMM1+RBP+40h],MASK=K2,PREFIX=MVEX,OPER=0 ; No conversion. |00000028:62F2793AC6540D20<1 | VGATHERPF1DPS [ZMM1+RBP+40h],MASK=K2,PREFIX=MVEX,OPER=3 ; {float16}. |00000030:62F2794AC6540D40 | VGATHERPF1DPS [ZMM1+RBP+40h],MASK=K2,PREFIX=MVEX,OPER=4 ; {uint8}. |00000038:62F2795AC6540D40 | VGATHERPF1DPS [ZMM1+RBP+40h],MASK=K2,PREFIX=MVEX,OPER=5 ; {sint8}. |00000040:62F2796AC6540D20<1 | VGATHERPF1DPS [ZMM1+RBP+40h],MASK=K2,PREFIX=MVEX,OPER=6 ; {uint16}. |00000048:62F2797AC6540D20<1 | VGATHERPF1DPS [ZMM1+RBP+40h],MASK=K2,PREFIX=MVEX,OPER=7 ; {sint16}. | |ENDPROGRAM t5446`

Expected messages t5446.out
  `I0180 Assembling source file "t5446.htm". I0270 Assembling source "t5446". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5446". "t5446.htm"{58} I0510 Assembling program pass 1. "t5446.htm"{58} I0530 Assembling program pass 2 - final. "t5446.htm"{58} I0660 16bit TINY BIN file "t5446.bin" created, size=80. "t5446.htm"{70} I0650 Program "t5446" assembled in 2 passes with errorlevel 0. "t5446.htm"{70} I0750 Source "t5446" (88 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5446.htm.lst" created, size=1200. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲