| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3750: Machine instructions MOVUPD MOVLPD MOVHPD MOVAPD MOVSS

Tested procedures
  IipMOVUPD IipMOVLPD IipMOVHPD IipMOVAPD IipMOVSS

Source & expected listing t3750.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=32, CPU=X64, SIMD=SSE2 | |t3750 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:660F120C | MOVLPD XMM1,[SI] |0004:660F130C | MOVLPD [SI],XMM1 |0008:660F160C | MOVHPD XMM1,[SI] |000C:660F170C | MOVHPD [SI],XMM1 |0010:660F28CF | MOVAPD XMM1,XMM7 |0014:660F28CF | MOVAPD XMM1,XMM7,CODE=SHORT |0018:660F29F9 | MOVAPD XMM1,XMM7,CODE=LONG |001C:660F280C | MOVAPD XMM1,[SI] |0020:660F290C | MOVAPD [SI],XMM1 |0024:660F10CF | MOVUPD XMM1,XMM7 |0028:660F10CF | MOVUPD XMM1,XMM7,CODE=SHORT |002C:660F11F9 | MOVUPD XMM1,XMM7,CODE=LONG |0030:660F100C | MOVUPD XMM1,[SI] |0034:660F110C | MOVUPD [SI],XMM1 |0038:F30F10CF | MOVSS XMM1,XMM7 |003C:F30F10CF | MOVSS XMM1,XMM7,CODE=SHORT |0040:F30F11F9 | MOVSS XMM1,XMM7,CODE=LONG |0044:F30F100C | MOVSS XMM1,[SI] |0048:26F30F110C | MOVSS [ES:SI],XMM1 |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:660F120E | MOVLPD XMM1,[ESI] |00000004:660F130E | MOVLPD [ESI],XMM1 |00000008:66670F160C | MOVHPD XMM1,[SI] |0000000D:660F170E | MOVHPD [ESI],XMM1 |00000011:660F28CF | MOVAPD XMM1,XMM7 |00000015:660F28CF | MOVAPD XMM1,XMM7,CODE=SHORT |00000019:660F29F9 | MOVAPD XMM1,XMM7,CODE=LONG |0000001D:66670F280C | MOVAPD XMM1,[SI] |00000022:660F290E | MOVAPD [ESI],XMM1 |00000026:660F10CF | MOVUPD XMM1,XMM7 |0000002A:660F10CF | MOVUPD XMM1,XMM7,CODE=SHORT |0000002E:660F11F9 | MOVUPD XMM1,XMM7,CODE=LONG |00000032:66670F100C | MOVUPD XMM1,[SI] |00000037:660F110E | MOVUPD [ESI],XMM1 |0000003B:F30F10CF | MOVSS XMM1,XMM7 |0000003F:F30F10CF | MOVSS XMM1,XMM7,CODE=SHORT |00000043:F30F11F9 | MOVSS XMM1,XMM7,CODE=LONG |00000047:67F30F100C | MOVSS XMM1,[SI] |0000004C:F30F110E | MOVSS [ESI],XMM1 |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:66670F120E | MOVLPD XMM1,[ESI] |00000005:66440F133E | MOVLPD [RSI],XMM15 |0000000A:660F160E | MOVHPD XMM1,[RSI] |0000000E:660F170E | MOVHPD [RSI],XMM1 |00000012:66450F28DF | MOVAPD XMM11,XMM15 |00000017:66450F28DF | MOVAPD XMM11,XMM15,CODE=SHORT |0000001C:66450F29FB | MOVAPD XMM11,XMM15,CODE=LONG |00000021:660F280E | MOVAPD XMM1,[RSI] |00000025:660F290E | MOVAPD [RSI],XMM1 |00000029:660F10CF | MOVUPD XMM1,XMM7 |0000002D:660F10CF | MOVUPD XMM1,XMM7,CODE=SHORT |00000031:660F11F9 | MOVUPD XMM1,XMM7,CODE=LONG |00000035:660F100C2500000000 | MOVUPD XMM1,[0] |0000003E:66440F111C2500000000 | MOVUPD [0],XMM11 |00000048:F30F10CF | MOVSS XMM1,XMM7 |0000004C:F30F10CF | MOVSS XMM1,XMM7,CODE=SHORT |00000050:F30F11F9 | MOVSS XMM1,XMM7,CODE=LONG |00000054:F3440F107D10 | MOVSS XMM15,[RBP+16] |0000005A:67F3440F117DF0 | MOVSS [EBP-16],XMM15 | |ENDPROGRAM t3750`

Expected messages t3750.out
  `I0180 Assembling source file "t3750.htm". I0270 Assembling source "t3750". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3750". "t3750.htm"{61} I0510 Assembling program pass 1. "t3750.htm"{61} I0530 Assembling program pass 2 - final. "t3750.htm"{61} I0660 16bit TINY BIN file "t3750.bin" created, size=257. "t3750.htm"{122} I0650 Program "t3750" assembled in 2 passes with errorlevel 0. "t3750.htm"{122} I0750 Source "t3750" (140 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3750.htm.lst" created, size=3565. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲