| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3056: Machine instructions SAL2 SAL2B SAL2W SAL2D in 16bit mode

Tested procedures
  IigSAL2 IigSAL2B IigSAL2W IigSAL2D

Source & expected listing t3056.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=36,CPU=386 | |t3056 PROGRAM FORMAT=BIN,IMAGEBASE=0,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE | | EUROASM UNDOC=ENABLE |0000:D2F0 | SAL2 AL,CL |0002:D0F0 | SAL2 AL |0004:D0F0 | SAL2 AL,1 |0006:C0F001 | SAL2 AL,1,CODE=LONG |0009:C0F001 | SAL2 AL,1,IMM=BYTE |000C:C0F002 | SAL2 AL,2 |000F:D236[AE00] | SAL2 [MemByte],CL |0013:D036[AE00] | SAL2 [MemByte] |0017:D036[AE00] | SAL2 [MemByte],1 |001B:C036[AE00]01 | SAL2 [MemByte],1,CODE=LONG |0020:C036[AE00]01 | SAL2 [MemByte],1,IMM=BYTE |0025:C036[AE00]02 | SAL2 [MemByte],2 |002A:C03501 | SAL2 [DI],1,DATA=BYTE,IMM=BYTE |002D:67D037 | SAL2 [EDI],1,DATA=BYTE |0030:D3F0 | SAL2 AX,CL |0032:D1F0 | SAL2 AX |0034:D1F0 | SAL2 AX,1 |0036:C1F001 | SAL2 AX,1,CODE=LONG |0039:C1F001 | SAL2 AX,1,IMM=BYTE |003C:C1F002 | SAL2 AX,2 |003F:D336[AC00] | SAL2 [MemWord],CL |0043:D136[AC00] | SAL2 [MemWord] |0047:D136[AC00] | SAL2 [MemWord],1 |004B:C136[AC00]01 | SAL2 [MemWord],1,CODE=LONG |0050:C136[AC00]01 | SAL2 [MemWord],1,IMM=BYTE |0055:C136[AC00]02 | SAL2 [MemWord],2 |005A:C13501 | SAL2 [DI],1,DATA=WORD,IMM=BYTE |005D:67D137 | SAL2 [EDI],1,DATA=WORD |0060:66D3F0 | SAL2 EAX,CL |0063:66D1F0 | SAL2 EAX |0066:66D1F0 | SAL2 EAX,1 |0069:66C1F001 | SAL2 EAX,1,CODE=LONG |006D:66C1F001 | SAL2 EAX,1,IMM=BYTE |0071:66C1F002 | SAL2 EAX,2 |0075:66D336[A800] | SAL2 [MemDword],CL |007A:66D136[A800] | SAL2 [MemDword] |007F:66D136[A800] | SAL2 [MemDword],1 |0084:66C136[A800]01 | SAL2 [MemDword],1,CODE=LONG |008A:66C136[A800]01 | SAL2 [MemDword],1,IMM=BYTE |0090:66C136[A800]02 | SAL2 [MemDword],2 |0096:66C13501 | SAL2 [DI],1,DATA=DWORD,IMM=BYTE |009A:6667D137 | SAL2 [EDI],1,DATA=DWORD |009E:D235 | SAL2B [DI],CL |00A0:D335 | SAL2W [DI],CL |00A2:66D335 | SAL2D [DI],CL |00A5:9087C9 | ALIGN QWORD |00A8:00000000 |MemDword D D |00AC:0000 |MemWord D W |00AE:00 |MemByte D B | |ENDPROGRAM t3056`

Expected messages t3056.out
  `I0180 Assembling source file "t3056.htm". I0270 Assembling source "t3056". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3056". "t3056.htm"{58} I0510 Assembling program pass 1. "t3056.htm"{58} I0510 Assembling program pass 2. "t3056.htm"{58} I0510 Assembling program pass 3. "t3056.htm"{58} I0530 Assembling program pass 4 - final. "t3056.htm"{58} I0660 16bit TINY BIN file "t3056.bin" created, size=175. "t3056.htm"{110} I0650 Program "t3056" assembled in 4 passes with errorlevel 0. "t3056.htm"{110} I0750 Source "t3056" (130 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3056.htm.lst" created, size=3096. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲