| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t4414: Machine instructions ENCLV ENDBR32 ENDBR64 HRESET SENDUIPI SERIALIZE UMONITOR UMWAIT

Description
  SGX instructions
Tested procedures
  IisENCLV IisENDBR32 IisENDBR64 IisHRESET IisSENDUIPI IisSERIALIZE IisUMONITOR IisUMWAIT

Source & expected listing t4414.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=32, CPU=686, PRIV=ENABLED, CET=ENABLED | |t4414 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF, IMAGEBASE=0 |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:0F01C0 | ENCLV |00000003:F30F1EFB | ENDBR32 |00000007:F30F3AF0C001 | HRESET 1 |0000000D:0F01E8 | SERIALIZE |00000010:F30FAEF0 | UMONITOR AX |00000014:F30FAEF0 | UMONITOR EAX |00000018:F20FAEF0 | UMWAIT EAX | |;; | | EUROASM CPU=X64 |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:0F01C0 | ENCLV |00000003:F30F1EFB | ENDBR32 |00000007:F30F1EFA | ENDBR64 |0000000B:F30F3AF0C001 | HRESET 1 |00000011:F30FC7F0 | SENDUIPI RAX |00000015:0F01E8 | SERIALIZE |00000018:F30FAEF0 | UMONITOR AX |0000001C:F30FAEF0 | UMONITOR EAX |00000020:F30FAEF0 | UMONITOR RAX |00000024:F20FAEF0 | UMWAIT EAX | |ENDPROGRAM t4414`

Expected messages t4414.out
  `I0180 Assembling source file "t4414.htm". I0270 Assembling source "t4414". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t4414". "t4414.htm"{73} I0510 Assembling program pass 1. "t4414.htm"{73} I0530 Assembling program pass 2 - final. "t4414.htm"{73} I0660 16bit TINY BIN file "t4414.bin" created, size=72. "t4414.htm"{95} I0650 Program "t4414" assembled in 2 passes with errorlevel 0. "t4414.htm"{95} I0750 Source "t4414" (113 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t4414.htm.lst" created, size=1245. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲