| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5632: Machine instructions VPSRLVW VPSRLVD VPSRLVQ

Tested procedures
  IizVPSRLVW IizVPSRLVD IizVPSRLVQ

Source & expected listing t5632.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON,MVEX=ON | |t5632 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F2ED0810CB | VPSRLVW XMM1,XMM2,XMM3 |00000006:62F2ED2C10CB | VPSRLVW YMM1,YMM2,YMM3,MASK=K4 |0000000C:62F2EDCC10CB | VPSRLVW ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000012:62F2ED08104D04<4 | VPSRLVW XMM1,XMM2,[RBP+40h] |00000019:62F2ED2C104D02<5 | VPSRLVW YMM1,YMM2,[RBP+40h],MASK=K4 |00000020:62F2EDCC104D01<6 | VPSRLVW ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000027:C4E26945CB | VPSRLVD XMM1,XMM2,XMM3 |0000002C:C4E26D45CB | VPSRLVD YMM1,YMM2,YMM3 |00000031:62F26D0C45CB | VPSRLVD XMM1,XMM2,XMM3,MASK=K4 |00000037:62F26D2C45CB | VPSRLVD YMM1,YMM2,YMM3,MASK=K4 |0000003D:62F26D4845CB | VPSRLVD ZMM1,ZMM2,ZMM3 |00000043:62F2692845CB | VPSRLVD ZMM1,ZMM2,ZMM3,EH=OFF,OPER=2 ; MVEX {badc}. |00000049:C4E269454D40 | VPSRLVD XMM1,XMM2,[RBP+40h] |0000004F:C4E26D454D40 | VPSRLVD YMM1,YMM2,[RBP+40h] |00000055:62F26D08454D04<4 | VPSRLVD XMM1,XMM2,[RBP+40h],BCST=OFF |0000005C:62F26D28454D02<5 | VPSRLVD YMM1,YMM2,[RBP+40h],BCST=OFF |00000063:62F26D48454D01<6 | VPSRLVD ZMM1,ZMM2,[RBP+40h],BCST=OFF |0000006A:62F26D18454D10<2 | VPSRLVD XMM1,XMM2,[RBP+40h],BCST=ON |00000071:62F26D38454D10<2 | VPSRLVD YMM1,YMM2,[RBP+40h],BCST=ON |00000078:62F26D58454D10<2 | VPSRLVD ZMM1,ZMM2,[RBP+40h],BCST=ON |0000007F:62F26908454D01<6 | VPSRLVD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=0 ; {16to16}. |00000086:62F26918454D10<2 | VPSRLVD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=1 ; {1to16}. |0000008D:62F26928454D04<4 | VPSRLVD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=2 ; {4to16}. |00000094:62F26948454D04<4 | VPSRLVD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=4 ; {uint8}. |0000009B:C4E2E945CB | VPSRLVQ XMM1,XMM2,XMM3 |000000A0:C4E2ED45CB | VPSRLVQ YMM1,YMM2,YMM3 |000000A5:62F2ED0C45CB | VPSRLVQ XMM1,XMM2,XMM3,MASK=K4 |000000AB:62F2ED2C45CB | VPSRLVQ YMM1,YMM2,YMM3,MASK=K4 |000000B1:62F2ED4845CB | VPSRLVQ ZMM1,ZMM2,ZMM3 |000000B7:C4E2E9454D40 | VPSRLVQ XMM1,XMM2,[RBP+40h] |000000BD:C4E2ED454D40 | VPSRLVQ YMM1,YMM2,[RBP+40h] |000000C3:62F2ED0C454D04<4 | VPSRLVQ XMM1,XMM2,[RBP+40h],MASK=K4 |000000CA:62F2ED2C454D02<5 | VPSRLVQ YMM1,YMM2,[RBP+40h],MASK=K4 |000000D1:62F2ED48454D01<6 | VPSRLVQ ZMM1,ZMM2,[RBP+40h] | |ENDPROGRAM t5632`

Expected messages t5632.out
  `I0180 Assembling source file "t5632.htm". I0270 Assembling source "t5632". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5632". "t5632.htm"{55} I0510 Assembling program pass 1. "t5632.htm"{55} I0530 Assembling program pass 2 - final. "t5632.htm"{55} I0660 16bit TINY BIN file "t5632.bin" created, size=216. "t5632.htm"{91} I0650 Program "t5632" assembled in 2 passes with errorlevel 0. "t5632.htm"{91} I0750 Source "t5632" (109 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5632.htm.lst" created, size=2581. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲