| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3406: Machine instructions LAR LSL

Tested procedures
  IisLAR IisLSL

Source & expected listing t3406.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=35, CPU=X64, PROT=ON | |t3406 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:0F02CA | LAR CX,DX |0003:0F02CA | LAR CX,EDX |0006:0F020C | LAR CX,[SI] |0009:660F02CA | LAR ECX,DX |000D:660F02CA | LAR ECX,EDX |0011:660F020C | LAR ECX,[SI] |0015:66670F020E | LAR ECX,[ESI] |001A:0F03CA | LSL CX,DX |001D:0F03CA | LSL CX,EDX |0020:0F030C | LSL CX,[SI] |0023:660F03CA | LSL ECX,DX |0027:660F03CA | LSL ECX,EDX |002B:660F030C | LSL ECX,[SI] |002F:66670F030E | LSL ECX,[ESI] |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:660F02CA | LAR CX,DX |00000004:660F02CA | LAR CX,EDX |00000008:660F020E | LAR CX,[ESI] |0000000C:0F02CA | LAR ECX,DX |0000000F:0F02CA | LAR ECX,EDX |00000012:670F020C | LAR ECX,[SI] |00000016:660F03CA | LSL CX,DX |0000001A:660F03CA | LSL CX,EDX |0000001E:660F030E | LSL CX,[ESI] |00000022:0F03CA | LSL ECX,DX |00000025:0F03CA | LSL ECX,EDX |00000028:670F030C | LSL ECX,[SI] |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:660F02CA | LAR CX,DX |00000004:660F02CA | LAR CX,EDX |00000008:660F02CA | LAR CX,RDX |0000000C:660F020E | LAR CX,[RSI] |00000010:0F02CA | LAR ECX,DX |00000013:0F02CA | LAR ECX,EDX |00000016:0F02CA | LAR ECX,RDX |00000019:670F020E | LAR ECX,[ESI] |0000001D:67420F020C06 | LAR ECX,[ESI+R8D] |00000023:480F02CA | LAR RCX,DX |00000027:480F02CA | LAR RCX,EDX |0000002B:480F02CA | LAR RCX,RDX |0000002F:490F02CA | LAR RCX,R10W |00000033:490F02CA | LAR RCX,R10D |00000037:490F02CA | LAR RCX,R10 |0000003B:480F020E | LAR RCX,[RSI] |0000003F:4A0F020C06 | LAR RCX,[RSI+R8] |00000044:660F03CA | LSL CX,DX |00000048:660F03CA | LSL CX,EDX |0000004C:660F03CA | LSL CX,RDX |00000050:660F030E | LSL CX,[RSI] |00000054:0F03CA | LSL ECX,DX |00000057:0F03CA | LSL ECX,EDX |0000005A:0F03CA | LSL ECX,RDX |0000005D:670F030E | LSL ECX,[ESI] |00000061:67420F030C06 | LSL ECX,[ESI+R8D] |00000067:480F03CA | LSL RCX,DX |0000006B:480F03CA | LSL RCX,EDX |0000006F:480F03CA | LSL RCX,RDX |00000073:490F03CA | LSL RCX,R10W |00000077:490F03CA | LSL RCX,R10D |0000007B:490F03CA | LSL RCX,R10 |0000007F:480F030E | LSL RCX,[RSI] |00000083:4A0F030C06 | LSL RCX,[RSI+R8] | | ENDPROGRAM t3406`

Expected messages t3406.out
  `I0180 Assembling source file "t3406.htm". I0270 Assembling source "t3406". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3406". "t3406.htm"{52} I0510 Assembling program pass 1. "t3406.htm"{52} I0530 Assembling program pass 2 - final. "t3406.htm"{52} I0660 16bit TINY BIN file "t3406.bin" created, size=248. "t3406.htm"{116} I0650 Program "t3406" assembled in 2 passes with errorlevel 0. "t3406.htm"{116} I0750 Source "t3406" (134 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3406.htm.lst" created, size=3423. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲