| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3132: Machine instructions NOP NOP1 NOP2 NOP3 NOP4 NOP5 NOP6 NOP7 NOP8 NOP9 in 32bit mode

Tested procedures
  IisNOP IisNOP1 IisNOP2 IisNOP3 IisNOP4 IisNOP5 IisNOP6 IisNOP7 IisNOP8 IisNOP9

Source & expected listing t3132.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=30 | |t3132 PROGRAM FORMAT=BIN,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE | | EUROASM CPU=386 |00000000:90 | NOP |00000001:90 | NOP1 |00000002:6690 | NOP2 |00000004:8D4000 | NOP3 |00000007:8D442000 | NOP4 |0000000B:3E8D442000 | NOP5 |00000010:8D8000000000 | NOP6 |00000016:8D842000000000 | NOP7 |0000001D:3E8D842000000000 | NOP8 |00000025:663E8D842000000000 | NOP9 | | EUROASM CPU=686 |0000002E:90 | NOP |0000002F:6690 | OTOGGLE NOP |00000031:0F1F00 | NOP [EAX],DATA=DWORD |00000034:0F1F4000 | NOP [EAX],DATA=DWORD,DISP=BYTE |00000038:0F1F442000 | NOP [EAX+0*EAX],DATA=DWORD,SCALE=VERBATIM,DISP=BYTE |0000003D:660F1F442000 | NOP [EAX+0*EAX],DATA=WORD,SCALE=VERBATIM,DISP=BYTE |00000043:0F1F8000000000 | NOP [EAX],DATA=DWORD,DISP=DWORD |0000004A:0F1F842000000000 | NOP [EAX+0*EAX],DATA=DWORD,SCALE=VERBATIM,DISP=DWORD |00000052:660F1F842000000000 | NOP [EAX+0*EAX],DATA=WORD,SCALE=VERBATIM,DISP=DWORD |0000005B:90 | NOP1 |0000005C:6690 | NOP2 |0000005E:0F1F00 | NOP3 |00000061:0F1F4000 | NOP4 |00000065:0F1F442000 | NOP5 |0000006A:660F1F442000 | NOP6 |00000070:0F1F8000000000 | NOP7 |00000077:0F1F842000000000 | NOP8 |0000007F:660F1F842000000000 | NOP9 | |ENDPROGRAM t3132`

Expected messages t3132.out
  `I0180 Assembling source file "t3132.htm". I0270 Assembling source "t3132". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3132". "t3132.htm"{76} I0510 Assembling program pass 1. "t3132.htm"{76} I0530 Assembling program pass 2 - final. "t3132.htm"{76} I0660 16bit TINY BIN file "t3132.bin" created, size=136. "t3132.htm"{108} I0650 Program "t3132" assembled in 2 passes with errorlevel 0. "t3132.htm"{108} I0750 Source "t3132" (126 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3132.htm.lst" created, size=1668. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲