| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t6128: Machine instructions VSCALEPS VADDNPS VADDNPD

Tested procedures
  IiyVSCALEPS IiyVADDNPS IiyVADDNPD

Source & expected listing t6128.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,MVEX=ON | |t6128 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F2690C84CB | VSCALEPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=0 ; {dcba}. |00000006:62F2691C84CB | VSCALEPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=1 ; {cdab}. |0000000C:62F2692C84CB | VSCALEPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=2 ; {badc}. |00000012:62F2693C84CB | VSCALEPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=3 ; {dacb}. |00000018:62F2694C84CB | VSCALEPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=4 ; {aaaa}. |0000001E:62F2695C84CB | VSCALEPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=5 ; {bbbb}. |00000024:62F2696C84CB | VSCALEPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=6 ; {cccc}. |0000002A:62F2697C84CB | VSCALEPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=7 ; {dddd}. |00000030:62F2698C84CB | VSCALEPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=1,OPER=0 ; {rn}. |00000036:62F2699C84CB | VSCALEPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=1,OPER=1 ; {rd}. |0000003C:62F269AC84CB | VSCALEPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=1,OPER=2 ; {ru}. |00000042:62F269BC84CB | VSCALEPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=1,OPER=3 ; {rz}. |00000048:62F269CC84CB | VSCALEPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=1,OPER=4 ; {rn-sae}. |0000004E:62F269DC84CB | VSCALEPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=1,OPER=5 ; {rd-sae}. |00000054:62F269EC84CB | VSCALEPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=1,OPER=6 ; {ru-sae}. |0000005A:62F269FC84CB | VSCALEPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=1,OPER=7 ; {rz-sae}. |00000060:62F269FC84CB | VSCALEPS ZMM1,ZMM2,ZMM3,MASK=K4,ROUND=Z,SAE=ON |00000066:62F269BC84CB | VSCALEPS ZMM1,ZMM2,ZMM3,MASK=K4,ROUND=Z,SAE=OFF |0000006C:62F2690C844D01<6 | VSCALEPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=0 ; {16to16}. |00000073:62F2691C844D10<2 | VSCALEPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=1 ; {1to16}. |0000007A:62F2692C844D04<4 | VSCALEPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=2 ; {4to16}. |00000081:62F2694C844D04<4 | VSCALEPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=4 ; {uint8}. |00000088:62F2695C844D04<4 | VSCALEPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=5 ; {sint8}. |0000008F:62F2696C844D02<5 | VSCALEPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=6 ; {uint16}. |00000096:62F2697C844D02<5 | VSCALEPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=7 ; {sint16}. |0000009D:62F2691C50CB | VADDNPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=1 ; {cdab}. |000000A3:62F2690C504D01<6 | VADDNPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=0 ; {16to16}. |000000AA:62F2E91C50CB | VADDNPD ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=1 ; {cdab}. |000000B0:62F2E92C504D02<5 | VADDNPD ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=2 ; {1to16}. | |ENDPROGRAM t6128`

Expected messages t6128.out
  `I0180 Assembling source file "t6128.htm". I0270 Assembling source "t6128". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t6128". "t6128.htm"{55} I0510 Assembling program pass 1. "t6128.htm"{55} I0530 Assembling program pass 2 - final. "t6128.htm"{55} I0660 16bit TINY BIN file "t6128.bin" created, size=183. "t6128.htm"{86} I0650 Program "t6128" assembled in 2 passes with errorlevel 0. "t6128.htm"{86} I0750 Source "t6128" (104 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t6128.htm.lst" created, size=2791. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲