| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3071: Machine instructions ROR RORB RORW RORD RORQ in 64bit mode

Tested procedures
  IigROR IigRORB IigRORW IigRORD IigRORQ

Source & expected listing t3071.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=36,CPU=X64 | |t3071 PROGRAM FORMAT=BIN,IMAGEBASE=0,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:D2C8 | ROR AL,CL |00000002:D0C8 | ROR AL |00000004:D0C8 | ROR AL,1 |00000006:C0C801 | ROR AL,1,CODE=LONG |00000009:C0C801 | ROR AL,1,IMM=BYTE |0000000C:C0C802 | ROR AL,2 |0000000F:D20D19010000 | ROR [MemByte],CL |00000015:D00D13010000 | ROR [MemByte] |0000001B:D00D0D010000 | ROR [MemByte],1 |00000021:C00D0601000001 | ROR [MemByte],1,CODE=LONG |00000028:C00DFF00000001 | ROR [MemByte],1,IMM=BYTE |0000002F:C00DF800000002 | ROR [MemByte],2 |00000036:C00F01 | ROR [RDI],1,DATA=BYTE,IMM=BYTE |00000039:67D00F | ROR [EDI],1,DATA=BYTE |0000003C:66D3C8 | ROR AX,CL |0000003F:66D1C8 | ROR AX |00000042:66D1C8 | ROR AX,1 |00000045:66C1C801 | ROR AX,1,CODE=LONG |00000049:66C1C801 | ROR AX,1,IMM=BYTE |0000004D:66C1C802 | ROR AX,2 |00000051:66D30DD4000000 | ROR [MemWord],CL |00000058:66D10DCD000000 | ROR [MemWord] |0000005F:66D10DC6000000 | ROR [MemWord],1 |00000066:66C10DBE00000001 | ROR [MemWord],1,CODE=LONG |0000006E:66C10DB600000001 | ROR [MemWord],1,IMM=BYTE |00000076:66C10DAE00000002 | ROR [MemWord],2 |0000007E:66C10F01 | ROR [RDI],1,DATA=WORD,IMM=BYTE |00000082:6667D10F | ROR [EDI],1,DATA=WORD |00000086:D3C8 | ROR EAX,CL |00000088:D1C8 | ROR EAX |0000008A:D1C8 | ROR EAX,1 |0000008C:C1C801 | ROR EAX,1,CODE=LONG |0000008F:C1C801 | ROR EAX,1,IMM=BYTE |00000092:C1C802 | ROR EAX,2 |00000095:D30D8D000000 | ROR [MemDword],CL |0000009B:D10D87000000 | ROR [MemDword] |000000A1:D10D81000000 | ROR [MemDword],1 |000000A7:C10D7A00000001 | ROR [MemDword],1,CODE=LONG |000000AE:C10D7300000001 | ROR [MemDword],1,IMM=BYTE |000000B5:C10D6C00000002 | ROR [MemDword],2 |000000BC:67C10F01 | ROR [EDI],1,DATA=DWORD,IMM=BYTE |000000C0:D10F | ROR [RDI],1,DATA=DWORD |000000C2:48D3C8 | ROR RAX,CL |000000C5:48D1C8 | ROR RAX |000000C8:48D1C8 | ROR RAX,1 |000000CB:48C1C801 | ROR RAX,1,CODE=LONG |000000CF:48C1C801 | ROR RAX,1,IMM=BYTE |000000D3:48C1C802 | ROR RAX,2 |000000D7:48D30D42000000 | ROR [MemQword],CL |000000DE:48D10D3B000000 | ROR [MemQword] |000000E5:48D10D34000000 | ROR [MemQword],1 |000000EC:48C10D2C00000001 | ROR [MemQword],1,CODE=LONG |000000F4:48C10D2400000001 | ROR [MemQword],1,IMM=BYTE |000000FC:48C10D1C00000002 | ROR [MemQword],2 |00000104:6741C10801 | ROR [R8D],1,DATA=DWORD,IMM=BYTE |00000109:41D10C24 | ROR [R12],1,DATA=DWORD |0000010D:4AD14CA500 | ROR [RBP+4*R12],1,DATA=QWORD |00000112:D20F | RORB [RDI],CL |00000114:66D30F | RORW [RDI],CL |00000117:D30F | RORD [RDI],CL |00000119:48D30F | RORQ [RDI],CL |0000011C:0F1F4000 | ALIGN QWORD |00000120:0000000000000000 |MemQword D Q |00000128:00000000 |MemDword D D |0000012C:0000 |MemWord D W |0000012E:00 |MemByte D B | |ENDPROGRAM t3071`

Expected messages t3071.out
  `I0180 Assembling source file "t3071.htm". I0270 Assembling source "t3071". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3071". "t3071.htm"{61} I0510 Assembling program pass 1. "t3071.htm"{61} I0510 Assembling program pass 2. "t3071.htm"{61} I0510 Assembling program pass 3. "t3071.htm"{61} I0530 Assembling program pass 4 - final. "t3071.htm"{61} I0660 16bit TINY BIN file "t3071.bin" created, size=303. "t3071.htm"{129} I0650 Program "t3071" assembled in 4 passes with errorlevel 0. "t3071.htm"{129} I0750 Source "t3071" (149 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3071.htm.lst" created, size=3952. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲