| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5476: Machine instructions VMOVAPS VMOVAPD

Tested procedures
  IizVMOVAPS IizVMOVAPD

Source & expected listing t5476.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON,MVEX=ON | |t5476 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C5F828CA | VMOVAPS XMM1,XMM2 |00000004:C5F829D1 | VMOVAPS XMM1,XMM2,CODE=LONG |00000008:C4E17829D1 | VMOVAPS XMM1,XMM2,CODE=LONG,PREFIX=VEX3 |0000000D:62F17CAB28CA | VMOVAPS YMM1,YMM2,MASK=K3,ZEROING=ON,CODE=SHORT |00000013:62F17CAB29D1 | VMOVAPS YMM1,YMM2,MASK=K3,ZEROING=ON,CODE=LONG |00000019:62F17C4B28CA | VMOVAPS ZMM1,ZMM2,MASK=K3 |0000001F:62F17C4B29D1 | VMOVAPS ZMM1,ZMM2,MASK=K3,CODE=LONG |00000025:62F1780B28CA | VMOVAPS ZMM1,ZMM2,MASK=K3,PREFIX=MVEX,OPER=0 ; {dcba}. |0000002B:62F1782B28CA | VMOVAPS ZMM1,ZMM2,MASK=K3,PREFIX=MVEX,OPER=2 ; {badc}. |00000031:62F1784B28CA | VMOVAPS ZMM1,ZMM2,MASK=K3,PREFIX=MVEX,OPER=4 ; {aaaa}. |00000037:C5F8284D40 | VMOVAPS XMM1,[RBP+40h] |0000003C:C5F8294D40 | VMOVAPS [RBP+40h],XMM1 |00000041:62F17CAB284D02<5 | VMOVAPS YMM1,[RBP+40h],MASK=K3,ZEROING=ON |00000048:62F17CAB294D02<5 | VMOVAPS [RBP+40h],YMM1,MASK=K3,ZEROING=ON |0000004F:62F17C4B284D01<6 | VMOVAPS ZMM1,[RBP+40h],MASK=K3 |00000056:62F17CCB294D01<6 | VMOVAPS [RBP+40h],ZMM1,MASK=K3,ZEROING=ON |0000005D:62F1788B294D01<6 | VMOVAPS [RBP+40h],ZMM1,MASK=K3,EH=ON |00000064:62F1780B294D01<6 | VMOVAPS [RBP+40h],ZMM1,MASK=K3,PREFIX=MVEX,OPER=0 ; No conversion. |0000006B:62F1784B294D04<4 | VMOVAPS [RBP+40h],ZMM1,MASK=K3,PREFIX=MVEX,OPER=4 ; {uint8}. |00000072:62F1787B284D02<5 | VMOVAPS ZMM1,[RBP+40h],MASK=K3,PREFIX=MVEX,OPER=7 ; {sint16}. |00000079:62F1787B294D02<5 | VMOVAPS [RBP+40h],ZMM1,MASK=K3,PREFIX=MVEX,OPER=7 ; {sint16}. |00000080:C5F928CA | VMOVAPD XMM1,XMM2 |00000084:C5F929D1 | VMOVAPD XMM1,XMM2,CODE=LONG |00000088:C4E17929D1 | VMOVAPD XMM1,XMM2,CODE=LONG,PREFIX=VEX3 |0000008D:62F1FDAB28CA | VMOVAPD YMM1,YMM2,MASK=K3,ZEROING=ON,CODE=SHORT |00000093:62F1FDAB29D1 | VMOVAPD YMM1,YMM2,MASK=K3,ZEROING=ON,CODE=LONG |00000099:62F1FD4B28CA | VMOVAPD ZMM1,ZMM2,MASK=K3 |0000009F:62F1FD4B29D1 | VMOVAPD ZMM1,ZMM2,MASK=K3,CODE=LONG |000000A5:62F1F90B28CA | VMOVAPD ZMM1,ZMM2,MASK=K3,PREFIX=MVEX,OPER=0 ; {dcba}. |000000AB:62F1F92B28CA | VMOVAPD ZMM1,ZMM2,MASK=K3,PREFIX=MVEX,OPER=2 ; {badc}. |000000B1:62F1F94B28CA | VMOVAPD ZMM1,ZMM2,MASK=K3,PREFIX=MVEX,OPER=4 ; {aaaa}. |000000B7:C5F9284D40 | VMOVAPD XMM1,[RBP+40h] |000000BC:C5F9294D40 | VMOVAPD [RBP+40h],XMM1 |000000C1:62F1FDAB284D02<5 | VMOVAPD YMM1,[RBP+40h],MASK=K3,ZEROING=ON |000000C8:62F1FDAB294D02<5 | VMOVAPD [RBP+40h],YMM1,MASK=K3,ZEROING=ON |000000CF:62F1FD4B284D01<6 | VMOVAPD ZMM1,[RBP+40h],MASK=K3 |000000D6:62F1FDCB294D01<6 | VMOVAPD [RBP+40h],ZMM1,MASK=K3,ZEROING=ON |000000DD:62F1F98B294D01<6 | VMOVAPD [RBP+40h],ZMM1,MASK=K3,EH=ON |000000E4:62F1F90B294D01<6 | VMOVAPD [RBP+40h],ZMM1,MASK=K3,PREFIX=MVEX,OPER=0 ; No conversion. | |ENDPROGRAM t5476`

Expected messages t5476.out
  `I0180 Assembling source file "t5476.htm". I0270 Assembling source "t5476". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5476". "t5476.htm"{52} I0510 Assembling program pass 1. "t5476.htm"{52} I0530 Assembling program pass 2 - final. "t5476.htm"{52} I0660 16bit TINY BIN file "t5476.bin" created, size=235. "t5476.htm"{93} I0650 Program "t5476" assembled in 2 passes with errorlevel 0. "t5476.htm"{93} I0750 Source "t5476" (111 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5476.htm.lst" created, size=3171. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲