| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3302: Machine instructions Jcc in 32bit mode

Description
  Conditional jumps
Tested procedures
  IigJcc

Source & expected listing t3302.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=33, CPU=386 | |t3302 PROGRAM FORMAT=OMF,MODEL=TINY,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:7070 | JO ShortLabel: |00000002:0F806A000000 | JO ShortLabel:,DIST=NEAR |00000008:7107EA[72000000]{0000}| JO ShortLabel:,DIST=FAR |00000011:0F8097000000 | JO NearLabel: |00000017:660F809200 | JO NearLabel:,DATA=WORD |0000001C:660F808D00 | JO NearLabel:,IMM=WORD |00000021:0F80(00000000) | JO FarLabel: |00000027:660F80(0000) | JO FarLabel:,DATA=WORD |0000002C:660F80(0000) | JO FarLabel:,IMM=WORD |00000031:0F80(00000000) | JO ExternLabel: |00000037:660F80(0000) | JO ExternLabel:,DATA=WORD |0000003C:660F80(0000) | JO ExternLabel:,IMM=WORD |00000041:0F80(77000000) | JO 0x77 |00000047:660F80(8877) | JO 0x7788,DATA=WORD |0000004C:0F80(99887700) | JO 0x778899 |00000052:0F807AFFFFFF | JO $-128 |00000058:0F807BFFFFFF | JO $-127 |0000005E:7080 | JO $-126 |00000060:7081 | JO $-125 |00000062:707E | JO $+128 |00000064:707F | JO $+129 |00000066:0F807C000000 | JO $+130 |0000006C:0F807D000000 | JO $+131 |00000072: |ShortLabel: |00000072:7000 | JO $+2 |00000074:7100 | JNO $+2 |00000076:7200 | JB $+2 |00000078:7200 | JC $+2 |0000007A:7200 | JNAE $+2 |0000007C:7300 | JAE $+2 |0000007E:7300 | JNB $+2 |00000080:7300 | JNC $+2 |00000082:7400 | JE $+2 |00000084:7400 | JZ $+2 |00000086:7500 | JNE $+2 |00000088:7500 | JNZ $+2 |0000008A:7600 | JBE $+2 |0000008C:7600 | JNA $+2 |0000008E:7700 | JA $+2 |00000090:7700 | JNBE $+2 |00000092:7800 | JS $+2 |00000094:7900 | JNS $+2 |00000096:7A00 | JP $+2 |00000098:7A00 | JPE $+2 |0000009A:7B00 | JNP $+2 |0000009C:7B00 | JPO $+2 |0000009E:7C00 | JL $+2 |000000A0:7C00 | JNGE $+2 |000000A2:7D00 | JGE $+2 |000000A4:7D00 | JNL $+2 |000000A6:7E00 | JLE $+2 |000000A8:7E00 | JNG $+2 |000000AA:7F00 | JG $+2 |000000AC:7F00 | JNLE $+2 |000000AE: |NearLabel: |[FarSeg] |[FarSeg] SEGMENT WIDTH=32,PURPOSE=CODE |00000000: |FarLabel: | |ExternLabel: EXTERN | |ENDPROGRAM t3302 |## W3831 Self-relative relocation to an absolute VA at [Mode32]:00000043h is not linkable. |## W3831 Self-relative relocation to an absolute VA at [Mode32]:0000004Ah is not linkable. |## W3831 Self-relative relocation to an absolute VA at [Mode32]:0000004Eh is not linkable.`

Expected messages t3302.out
  `I0180 Assembling source file "t3302.htm". I0270 Assembling source "t3302". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3302". "t3302.htm"{52} I0510 Assembling program pass 1. "t3302.htm"{52} I0510 Assembling program pass 2. "t3302.htm"{52} I0510 Assembling program pass 3. "t3302.htm"{52} I0530 Assembling program pass 4 - final. "t3302.htm"{52} I0623 Jcc out of byte range; assembled with proxy jump. "t3302.htm"{56} W3831 Self-relative relocation to an absolute VA at [Mode32]:00000043h is not linkable. "t3302.htm"{112} W3831 Self-relative relocation to an absolute VA at [Mode32]:0000004Ah is not linkable. "t3302.htm"{112} W3831 Self-relative relocation to an absolute VA at [Mode32]:0000004Eh is not linkable. "t3302.htm"{112} I0660 16bit TINY OMF file "t3302.obj" created, size=327. "t3302.htm"{112} I0650 Program "t3302" assembled in 4 passes with errorlevel 3. "t3302.htm"{112} I0750 Source "t3302" (139 lines) assembled in 2 passes with errorlevel 3. I0860 Listing file "t3302.htm.lst" created, size=3333. I0990 EuroAssembler terminated with errorlevel 3.`

▲Back to the top▲