| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t4522: Machine instructions VPMACSWW VPMACSWD VPMACSDQL VPMACSDD VPMACSDQH

Tested procedures
  IixVPMACSWW IixVPMACSWD IixVPMACSDQL IixVPMACSDD IixVPMACSDQH

Source & expected listing t4522.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=28,CPU=X64,SIMD=AVX,AMD=ON,XOP=ON,PROT=ON | |t4522 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:8FE86895CB40 | VPMACSWW XMM1,XMM2,XMM3,XMM4 |00000006:8FE868950E40 | VPMACSWW XMM1,XMM2,[RSI],XMM4 |0000000C:8FE86896CB40 | VPMACSWD XMM1,XMM2,XMM3,XMM4 |00000012:8FE868960E40 | VPMACSWD XMM1,XMM2,[RSI],XMM4 |00000018:8FE86897CB40 | VPMACSDQL XMM1,XMM2,XMM3,XMM4 |0000001E:8FE868970E40 | VPMACSDQL XMM1,XMM2,[RSI],XMM4 |00000024:8FE8689ECB40 | VPMACSDD XMM1,XMM2,XMM3,XMM4 |0000002A:8FE8689E0E40 | VPMACSDD XMM1,XMM2,[RSI],XMM4 |00000030:8FE8689FCB40 | VPMACSDQH XMM1,XMM2,XMM3,XMM4 |00000036:8FE8689F0E40 | VPMACSDQH XMM1,XMM2,[RSI],XMM4 |0000003C:8F48289FCBC0 | VPMACSDQH XMM9,XMM10,XMM11,XMM12 |00000042:678FA8689F0C4640 | VPMACSDQH XMM1,XMM2,[ESI+2*R8D],XMM4 | |ENDPROGRAM t4522`

Expected messages t4522.out
  `I0180 Assembling source file "t4522.htm". I0270 Assembling source "t4522". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t4522". "t4522.htm"{61} I0510 Assembling program pass 1. "t4522.htm"{61} I0530 Assembling program pass 2 - final. "t4522.htm"{61} I0660 16bit TINY BIN file "t4522.bin" created, size=74. "t4522.htm"{75} I0650 Program "t4522" assembled in 2 passes with errorlevel 0. "t4522.htm"{75} I0750 Source "t4522" (93 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t4522.htm.lst" created, size=1041. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲