| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5294: Machine instructions VPEXTRB VPEXTRW VPEXTRD VPEXTRQ

Tested procedures
  IizVPEXTRB IizVPEXTRW IizVPEXTRD IizVPEXTRQ

Source & expected listing t5294.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=34, DUMPALL=OFF, CPU=X64, SIMD=AVX512, EVEX=ON | |t5294 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C4E37914D003 | VPEXTRB AL,XMM2,3 |00000006:C4E37914D003 | VPEXTRB AX,XMM2,3 |0000000C:C4E37914D003 | VPEXTRB EAX,XMM2,3 |00000012:C4E37914D003 | VPEXTRB RAX,XMM2,3 |00000018:62F37D0814D003 | VPEXTRB RAX,XMM2,3,PREFIX=EVEX |0000001F:62E37D0814D003 | VPEXTRB RAX,XMM18,3 |00000026:C4E37914554003 | VPEXTRB [RBP+40h],XMM2,3 |0000002D:62F37D0814554003 | VPEXTRB [RBP+40h],XMM2,3,PREFIX=EVEX |00000035:C5F9C5C203 | VPEXTRW AX,XMM2,3 |0000003A:C5F9C5C203 | VPEXTRW EAX,XMM2,3 |0000003F:C5F9C5C203 | VPEXTRW RAX,XMM2,3 |00000044:C4E37915D003 | VPEXTRW RAX,XMM2,3,CODE=LONG |0000004A:C4E179C5C203 | VPEXTRW RAX,XMM2,3,PREFIX=VEX3 |00000050:62F17C08C5C203 | VPEXTRW RAX,XMM2,3,PREFIX=EVEX |00000057:62F37D0815D003 | VPEXTRW RAX,XMM2,3,PREFIX=EVEX,CODE=LONG |0000005E:62B17C08C5C203 | VPEXTRW RAX,XMM18,3 |00000065:C4E37915554003 | VPEXTRW [RBP+40h],XMM2,3 |0000006C:62F37D08155520<103 | VPEXTRW [RBP+40h],XMM2,3,PREFIX=EVEX |00000074:62E37D08155520<103 | VPEXTRW [RBP+40h],XMM18,3 |0000007C:C4E37916D003 | VPEXTRD EAX,XMM2,3 |00000082:C4E37916D003 | VPEXTRD RAX,XMM2,3 |00000088:62F37D0816D003 | VPEXTRD RAX,XMM2,3,PREFIX=EVEX |0000008F:62E37D0816D003 | VPEXTRD RAX,XMM18,3 |00000096:C4E37916554003 | VPEXTRD [RBP+40h],XMM2,3 |0000009D:62F37D08165510<203 | VPEXTRD [RBP+40h],XMM2,3,PREFIX=EVEX |000000A5:C4E3F916D003 | VPEXTRQ RAX,XMM2,3 |000000AB:62F3FD0816D003 | VPEXTRQ RAX,XMM2,3,PREFIX=EVEX |000000B2:62E3FD0816D003 | VPEXTRQ RAX,XMM18,3 |000000B9:C4E3F916554003 | VPEXTRQ [RBP+40h],XMM2,3 |000000C0:62F3FD08165508<303 | VPEXTRQ [RBP+40h],XMM2,3,PREFIX=EVEX | |ENDPROGRAM t5294`

Expected messages t5294.out
  `I0180 Assembling source file "t5294.htm". I0270 Assembling source "t5294". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5294". "t5294.htm"{58} I0510 Assembling program pass 1. "t5294.htm"{58} I0530 Assembling program pass 2 - final. "t5294.htm"{58} I0660 16bit TINY BIN file "t5294.bin" created, size=200. "t5294.htm"{90} I0650 Program "t5294" assembled in 2 passes with errorlevel 0. "t5294.htm"{90} I0750 Source "t5294" (108 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5294.htm.lst" created, size=2181. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲