| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3430: Machine instructions PREFETCH PREFETCHW PREFETCHNTA PREFETCHT0 PREFETCHT1 PREFETCHT2 PREFETCHWT1

Tested procedures
  IisPREFETCH IisPREFETCHW IisPREFETCHNTA IisPREFETCHT0 IisPREFETCHT1 IisPREFETCHT2 IisPREFETCHWT1

Source & expected listing t3430.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=28,CPU=X64,AMD=ON,D3NOW=ON | |t3430 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:0F0D04 | PREFETCH [SI] |0003:0F0D0C | PREFETCHW [SI] |0006:0F1804 | PREFETCHNTA [SI] |0009:0F180C | PREFETCHT0 [SI] |000C:0F1814 | PREFETCHT1 [SI] |000F:0F181C | PREFETCHT2 [SI] | | EUROASM UNDOC=ENABLED |0012:0F0D14 | PREFETCHWT1 [SI] |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:670F0D04 | PREFETCH [SI] |00000004:670F0D0C | PREFETCHW [SI] |00000008:670F1804 | PREFETCHNTA [SI] |0000000C:670F180C | PREFETCHT0 [SI] |00000010:670F1814 | PREFETCHT1 [SI] |00000014:670F181C | PREFETCHT2 [SI] |00000018:670F0D14 | PREFETCHWT1 [SI] |0000001C:0F0D06 | PREFETCH [ESI] |0000001F:0F0D0E | PREFETCHW [ESI] |00000022:0F1806 | PREFETCHNTA [ESI] |00000025:0F180E | PREFETCHT0 [ESI] |00000028:0F1816 | PREFETCHT1 [ESI] |0000002B:0F181E | PREFETCHT2 [ESI] |0000002E:0F0D16 | PREFETCHWT1 [ESI] |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:0F0D06 | PREFETCH [RSI] |00000003:0F0D0E | PREFETCHW [RSI] |00000006:0F1806 | PREFETCHNTA [RSI] |00000009:670F180C1E | PREFETCHT0 [ESI+EBX] |0000000E:67420F18141E | PREFETCHT1 [ESI+R11D] |00000014:0F181C2500000000 | PREFETCHT2 [0] |0000001C:410F0D13 | PREFETCHWT1 [R11] | |ENDPROGRAM t3430`

Expected messages t3430.out
  `I0180 Assembling source file "t3430.htm". I0270 Assembling source "t3430". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3430". "t3430.htm"{67} I0510 Assembling program pass 1. "t3430.htm"{67} I0530 Assembling program pass 2 - final. "t3430.htm"{67} I0660 16bit TINY BIN file "t3430.bin" created, size=128. "t3430.htm"{100} I0650 Program "t3430" assembled in 2 passes with errorlevel 0. "t3430.htm"{100} I0750 Source "t3430" (118 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3430.htm.lst" created, size=1783. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲