| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3730: Machine instructions PINSRB, PINSRW, PINSRD, PINSRQ

Tested procedures
  IipPINSRB IimPINSRW IipPINSRD IipPINSRQ

Source & expected listing t3730.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=30, CPU=X64, SIMD=SSE4.1 | |t3730 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:660F3A20F901 | PINSRB XMM7,CL,1 |0006:660F3A20F901 | PINSRB XMM7,CX,1 |000C:660F3A20F901 | PINSRB XMM7,ECX,1 |0012:660F3A203C01 | PINSRB XMM7,[SI],1 |0018:660FC4F901 | PINSRW XMM7,CX,1 |001D:660FC4F901 | PINSRW XMM7,ECX,1 |0022:660FC43C01 | PINSRW XMM7,[SI],1 |0027:660F3A22F901 | PINSRD XMM7,ECX,1 |002D:660F3A223C01 | PINSRD XMM7,[SI],1 |0033:66670F3A223E01 | PINSRD XMM7,[ESI],1 |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:660F3A20F901 | PINSRB XMM7,CL,1 |00000006:660F3A20F901 | PINSRB XMM7,CX,1 |0000000C:660F3A20F901 | PINSRB XMM7,ECX,1 |00000012:660F3A203E01 | PINSRB XMM7,[ESI],1 |00000018:660FC4F901 | PINSRW XMM7,CX,1 |0000001D:660FC4F901 | PINSRW XMM7,ECX,1 |00000022:660FC43E01 | PINSRW XMM7,[ESI],1 |00000027:660F3A22F901 | PINSRD XMM7,ECX,1 |0000002D:66670F3A223C01 | PINSRD XMM7,[SI],1 |00000034:660F3A223E01 | PINSRD XMM7,[ESI],1 |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:660F3A20F901 | PINSRB XMM7,CL,1 |00000006:660F3A20F901 | PINSRB XMM7,CX,1 |0000000C:660F3A20F901 | PINSRB XMM7,ECX,1 |00000012:660F3A20F901 | PINSRB XMM7,RCX,1 |00000018:66440F3A20D901 | PINSRB XMM11,ECX,1 |0000001F:660F3A203E01 | PINSRB XMM7,[RSI],1 |00000025:66670F3A203E01 | PINSRB XMM7,[ESI],1 |0000002C:660FC4F901 | PINSRW XMM7,CX,1 |00000031:660FC4F901 | PINSRW XMM7,ECX,1 |00000036:660FC4F901 | PINSRW XMM7,RCX,1 |0000003B:6667460FC41C0E01 | PINSRW XMM11,[ESI+R9D],1 |00000043:660F3A22F901 | PINSRD XMM7,ECX,1 |00000049:660F3A22F901 | PINSRD XMM7,RCX,1 |0000004F:66420F3A223C1E01 | PINSRD XMM7,[RSI+R11],1 |00000057:66670F3A223E01 | PINSRD XMM7,[ESI],1 |0000005E:66670F3A223E01 | PINSRD XMM7,[ESI],1 |00000065:66460F3A221C1E01 | PINSRD XMM11,[RSI+R11],1 |0000006D:66480F3A22F901 | PINSRQ XMM7,RCX,1 |00000074:664A0F3A223C1E01 | PINSRQ XMM7,[RSI+R11],1 |0000007C:664E0F3A221C1E01 | PINSRQ XMM11,[RSI+R11],1 |00000084:6667480F3A223E01 | PINSRQ XMM7,[ESI],1 |0000008C:66674C0F3A221E01 | PINSRQ XMM11,[ESI],1 |00000094:66674E0F3A221C1E01 | PINSRQ XMM11,[ESI+R11D],1 | |ENDPROGRAM t3730`

Expected messages t3730.out
  `I0180 Assembling source file "t3730.htm". I0270 Assembling source "t3730". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3730". "t3730.htm"{58} I0510 Assembling program pass 1. "t3730.htm"{58} I0530 Assembling program pass 2 - final. "t3730.htm"{58} I0660 16bit TINY BIN file "t3730.bin" created, size=285. "t3730.htm"{105} I0650 Program "t3730" assembled in 2 passes with errorlevel 0. "t3730.htm"{105} I0750 Source "t3730" (123 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3730.htm.lst" created, size=2646. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲