| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5730: Machine instructions VPAND VPANDD VPANDQ

Tested procedures
  IiyVPAND IiyVPANDD IiyVPANDQ

Source & expected listing t5730.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON,MVEX=ON | |t5730 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C5E9DBCB | VPAND XMM1,XMM2,XMM3 |00000004:C5EDDBCB | VPAND YMM1,YMM2,YMM3 |00000008:C5E9DB4D40 | VPAND XMM1,XMM2,[RBP+40h] |0000000D:C5EDDB4D40 | VPAND YMM1,YMM2,[RBP+40h] |00000012:62F16D08DBCB | VPANDD XMM1,XMM2,XMM3 |00000018:62F16D28DBCB | VPANDD YMM1,YMM2,YMM3 |0000001E:62F16D8CDBCB | VPANDD XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000024:62F16DACDBCB | VPANDD YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |0000002A:62F16DCCDBCB | VPANDD ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000030:62F1692CDBCB | VPANDD ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=2 ; MVEX {badc}. |00000036:62F1694CDBCB | VPANDD ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=4 ; MVEX {aaaa}. |0000003C:62F16D08DB4D04<4 | VPANDD XMM1,XMM2,[RBP+40h],BCST=OFF |00000043:62F16D28DB4D02<5 | VPANDD YMM1,YMM2,[RBP+40h],BCST=OFF |0000004A:62F16D48DB4D01<6 | VPANDD ZMM1,ZMM2,[RBP+40h],BCST=OFF |00000051:62F16D18DB4D10<2 | VPANDD XMM1,XMM2,[RBP+40h],BCST=ON |00000058:62F16D38DB4D10<2 | VPANDD YMM1,YMM2,[RBP+40h],BCST=ON |0000005F:62F16D58DB4D10<2 | VPANDD ZMM1,ZMM2,[RBP+40h],BCST=ON |00000066:62F16908DB4D01<6 | VPANDD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=0 ; {16to16}. |0000006D:62F16918DB4D10<2 | VPANDD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=1 ; {1to16}. |00000074:62F16928DB4D04<4 | VPANDD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=2 ; {4to16}. |0000007B:62F1ED8CDBCB | VPANDQ XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000081:62F1EDACDBCB | VPANDQ YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |00000087:62F1EDCCDBCB | VPANDQ ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |0000008D:62F1E92CDBCB | VPANDQ ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=2 ; MVEX {badc}. |00000093:62F1E94CDBCB | VPANDQ ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=4 ; MVEX {aaaa}. |00000099:62F1ED8CDB4D04<4 | VPANDQ XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=OFF |000000A0:62F1EDACDB4D02<5 | VPANDQ YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=OFF |000000A7:62F1EDCCDB4D01<6 | VPANDQ ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=OFF |000000AE:62F1ED9CDB4D08<3 | VPANDQ XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |000000B5:62F1EDBCDB4D08<3 | VPANDQ YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |000000BC:62F1EDDCDB4D08<3 | VPANDQ ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |000000C3:62F1E908DB4D01<6 | VPANDQ ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=0 ; {16to16}. |000000CA:62F1E918DB4D08<3 | VPANDQ ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=1 ; {1to16}. |000000D1:62F1E928DB4D02<5 | VPANDQ ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=2 ; {4to16}. | |ENDPROGRAM t5730`

Expected messages t5730.out
  `I0180 Assembling source file "t5730.htm". I0270 Assembling source "t5730". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5730". "t5730.htm"{55} I0510 Assembling program pass 1. "t5730.htm"{55} I0530 Assembling program pass 2 - final. "t5730.htm"{55} I0660 16bit TINY BIN file "t5730.bin" created, size=216. "t5730.htm"{91} I0650 Program "t5730" assembled in 2 passes with errorlevel 0. "t5730.htm"{91} I0750 Source "t5730" (109 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5730.htm.lst" created, size=2893. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲