| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3113: Machine instructions SBB SBBB SBBW SBBD in 32bit mode

Tested procedures
  IigSBB IigSBBB IigSBBW IigSBBD

Source & expected listing t3113.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=36,CPU=386 | |t3113 PROGRAM FORMAT=BIN,IMAGEBASE=0,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:1C02 | SBB AL,2 |00000002:80D802 | SBB AL,2,CODE=LONG |00000005:661D0200 | SBB AX,2 |00000009:6683D802 | SBB AX,2,CODE=LONG |0000000D:83D802 | SBB EAX,2 |00000010:1D02000000 | SBB EAX,2,CODE=SHORT |00000015:80D902 | SBB CL,2 |00000018:801D[AE000000]02 | SBB [MemByte],2 |0000001F:6683D902 | SBB CX,2 |00000023:6681D90200 | SBB CX,2,IMM=WORD |00000028:66831D[AC000000]02 | SBB [MemWord],2 |00000030:66811D[AC000000]0200 | SBB [MemWord],2,IMM=WORD |00000039:811D[AC000000]02000000 | SBBD [MemWord],2,IMM=DWORD |00000043:83D902 | SBB ECX,2 |00000046:81D902000000 | SBB ECX,2,IMM=DWORD |0000004C:831D[A8000000]02 | SBB [MemDword],2 |00000053:66831D[A8000000]02 | SBBW [MemDword],2 |0000005B:811D[A8000000]02000000 | SBB [MemDword],2,IMM=DWORD |00000065:801F02 | SBBB [EDI],2 |00000068:66831F02 | SBBW [EDI],2 |0000006C:831F02 | SBBD [EDI],2 |0000006F:18D1 | SBB CL,DL |00000071:1ACA | SBB CL,DL,CODE=LONG |00000073:18F5 | SBB CH,DH |00000075:1AEE | SBB CH,DH,CODE=LONG |00000077:6619D1 | SBB CX,DX |0000007A:661BCA | SBB CX,DX,CODE=LONG |0000007D:19D1 | SBB ECX,EDX |0000007F:1BCA | SBB ECX,EDX,CODE=LONG |00000081:1A0D[AE000000] | SBB CL,[MemByte] |00000087:661B0D[AC000000] | SBB CX,[MemWord] |0000008E:1B0D[A8000000] | SBB ECX,[MemDword] |00000094:1815[AE000000] | SBB [MemByte],DL |0000009A:661915[AC000000] | SBB [MemWord],DX |000000A1:1915[A8000000] | SBB [MemDword],EDX |000000A7:90 | ALIGN QWORD |000000A8:00000000 |MemDword D D |000000AC:0000 |MemWord D W |000000AE:00 |MemByte D B | |ENDPROGRAM t3113`

Expected messages t3113.out
  `I0180 Assembling source file "t3113.htm". I0270 Assembling source "t3113". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3113". "t3113.htm"{58} I0510 Assembling program pass 1. "t3113.htm"{58} I0510 Assembling program pass 2. "t3113.htm"{58} I0510 Assembling program pass 3. "t3113.htm"{58} I0530 Assembling program pass 4 - final. "t3113.htm"{58} I0660 16bit TINY BIN file "t3113.bin" created, size=175. "t3113.htm"{99} I0650 Program "t3113" assembled in 4 passes with errorlevel 0. "t3113.htm"{99} I0750 Source "t3113" (119 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3113.htm.lst" created, size=2413. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲