| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3882: Machine instructions CMPSS CMPEQSS CMPLTSS CMPLESS CMPUNORDSS CMPNEQSS CMPNLTSS CMPNLESS CMPORDSS

Tested procedures
  IipCMPEQSS IipCMPLTSS IipCMPLESS IipCMPUNORDSS IipCMPNEQSS IipCMPNLTSS IipCMPNLESS IipCMPORDSS

Source & expected listing t3882.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=32, CPU=X64, SIMD=SSE1 | |t3882 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:F30FC2CE00 | CMPEQSS XMM1,XMM6 |0005:F30FC2CE01 | CMPLTSS XMM1,XMM6 |000A:F30FC2CE02 | CMPLESS XMM1,XMM6 |000F:F30FC2CE03 | CMPUNORDSS XMM1,XMM6 |0014:F30FC2CE04 | CMPNEQSS XMM1,XMM6 |0019:F30FC2CE05 | CMPNLTSS XMM1,XMM6 |001E:F30FC2CE06 | CMPNLESS XMM1,XMM6 |0023:F30FC2CE07 | CMPORDSS XMM1,XMM6 |0028:F30FC2CE07 | CMPSS XMM1,XMM6,7 |002D:26F30FC20C07 | CMPSS XMM1,[ES:SI],7 |0033:67F30FC20E07 | CMPSS XMM1,[ESI],7 |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:F30FC2CE00 | CMPEQSS XMM1,XMM6 |00000005:F30FC2CE01 | CMPLTSS XMM1,XMM6 |0000000A:F30FC2CE02 | CMPLESS XMM1,XMM6 |0000000F:F30FC2CE03 | CMPUNORDSS XMM1,XMM6 |00000014:F30FC2CE04 | CMPNEQSS XMM1,XMM6 |00000019:F30FC2CE05 | CMPNLTSS XMM1,XMM6 |0000001E:F30FC2CE06 | CMPNLESS XMM1,XMM6 |00000023:F30FC2CE07 | CMPORDSS XMM1,XMM6 |00000028:F30FC2CE07 | CMPSS XMM1,XMM6,7 |0000002D:2667F30FC20C07 | CMPSS XMM1,[ES:SI],7 |00000034:F30FC20E07 | CMPSS XMM1,[ESI],7 |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:F3440FC2DE00 | CMPEQSS XMM11,XMM6 |00000006:F3440FC2DE01 | CMPLTSS XMM11,XMM6 |0000000C:F3440FC2DE02 | CMPLESS XMM11,XMM6 |00000012:F3440FC2DE03 | CMPUNORDSS XMM11,XMM6 |00000018:F3440FC2DE04 | CMPNEQSS XMM11,XMM6 |0000001E:F3440FC2DE05 | CMPNLTSS XMM11,XMM6 |00000024:F3440FC2DE06 | CMPNLESS XMM11,XMM6 |0000002A:F3440FC2DE07 | CMPORDSS XMM11,XMM6 |00000030:F3440FC2DE07 | CMPSS XMM11,XMM6,7 |00000036:F3440FC21E07 | CMPSS XMM11,[RSI],7 |0000003C:67F3440FC21E07 | CMPSS XMM11,[ESI],7 | |ENDPROGRAM t3882`

Expected messages t3882.out
  `I0180 Assembling source file "t3882.htm". I0270 Assembling source "t3882". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3882". "t3882.htm"{70} I0510 Assembling program pass 1. "t3882.htm"{70} I0530 Assembling program pass 2 - final. "t3882.htm"{70} I0660 16bit TINY BIN file "t3882.bin" created, size=195. "t3882.htm"{107} I0650 Program "t3882" assembled in 2 passes with errorlevel 0. "t3882.htm"{107} I0750 Source "t3882" (125 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3882.htm.lst" created, size=2303. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲